<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0.0063" y1="0.005" x2="71.1137" y2="0.005" width="0" layer="20"/>
<wire x1="71.1137" y1="0.005" x2="71.1137" y2="66.0349" width="0" layer="20"/>
<wire x1="71.1137" y1="66.0349" x2="0.0063" y2="66.035" width="0" layer="20"/>
<wire x1="0.0063" y1="66.035" x2="0.0063" y2="0.005" width="0" layer="20"/>
<text>1</text>
<text>HV9910</text>
<text>AC\</text>
<text>LED</text>
<text>+ve</text>
</plain>
<libraries>
<library name="diode">
<packages>
<package name="P2-15">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 5 mm, horizontal, grid 12.7 mm</description>
</package>
<package name="TO220ACS">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
2-lead molded, vertical</description>
</package>
</packages>
</library>
<library name="con-wago-500">
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
<package name="XC15B5">
<description>&lt;b&gt;X CAPACITOR&lt;/b&gt;&lt;p&gt;
body 17.5 x 5 mm, grid 15.24 mm</description>
</package>
<package name="RTRIM64W">
<description>&lt;b&gt;Trimm resistor&lt;/b&gt; Spectrol&lt;p&gt;
Cermet MIL-R-22097</description>
</package>
<package name="C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="0207/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 15mm</description>
</package>
<package name="0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
</packages>
</library>
<library name="supertex">
<packages>
<package name="SOIC-16NG">
<description>&lt;b&gt;16-Lead SOIC (Narrow Body) Package Outline (NG)&lt;/b&gt;&lt;p&gt;
9.90x3.90mm body, 1.75mm height (max), 1.27mm pitch&lt;br&gt;
Source: www.supertex.com .. led_driver_ics_SG.pdf</description>
</package>
</packages>
</library>
<library name="inductor-nkl">
<packages>
<package name="B8">
<description>Becher B8 (cup B8)   top view
ca. Maße (approx. dimensions):
ØxH [mm]: 18x9
RM (grid) [mm]: 16
manufactured by NKL®</description>
</package>
</packages>
</library>
<library name="varistor">
<packages>
<package name="R-7,5">
<description>&lt;b&gt;VARISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-power">
<packages>
<package name="TO220BV">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CON1" library="con-wago-500" package="W237-102" value="AC"/>
<element name="CON2" library="con-wago-500" package="W237-102" value="LED"/>
<element name="C2" library="rcl" package="E5-10,5" value="22uf 400v"/>
<element name="C3" library="rcl" package="XC15B5" value="1.0uf 400v"/>
<element name="R3" library="rcl" package="RTRIM64W" value="5K"/>
<element name="C5" library="rcl" package="C050-025X075" value="0.1uf 25v"/>
<element name="R1" library="rcl" package="0207/10" value="182K"/>
<element name="R2" library="rcl" package="0207/10" value="1K"/>
<element name="R5" library="rcl" package="0207/10" value="470K"/>
<element name="IC1" library="supertex" package="SOIC-16NG" value="HV9910BNG"/>
<element name="C4" library="rcl" package="E2,5-5" value="2.2uf 16v"/>
<element name="C6" library="rcl" package="C050-025X075" value="100pf"/>
<element name="R4" library="rcl" package="0207/2V" value="1K"/>
<element name="NTC" library="varistor" package="R-7,5" value="50 ohm"/>
<element name="C1" library="rcl" package="XC15B5" value="0.1uf 400v"/>
<element name="C7" library="rcl" package="XC15B5" value="0.47uf 400v"/>
<element name="Q1" library="transistor-power" package="TO220BV" value="STD7NM50N"/>
<element name="D2" library="diode" package="P2-15" value="FR307"/>
<element name="D3" library="diode" package="P2-15" value="FR307"/>
<element name="D5" library="diode" package="P2-15" value="FR307"/>
<element name="D4" library="diode" package="P2-15" value="FR307"/>
<element name="D1" library="diode" package="TO220ACS" value="STTH2R06U"/>
<element name="L2" library="inductor-nkl" package="B8" value="1.0mH"/>
<element name="L1" library="inductor-nkl" package="B8" value="1.0mH"/>
<element name="R7" library="rcl" package="0207/15" value="0.22R"/>
<element name="R6" library="rcl" package="0207/5V" value="1K"/>
</elements>
<signals>
<signal name="N$5">
<contactref element="C2" pad="+"/>
<contactref element="C3" pad="1"/>
<contactref element="CON2" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="NTC" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="1"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="8"/>
<contactref element="Q1" pad="G"/>
</signal>
<signal name="N$13">
<contactref element="Q1" pad="D"/>
<contactref element="D1" pad="A"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="CON2" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="-"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="C4" pad="-"/>
<contactref element="C6" pad="2"/>
<contactref element="D5" pad="A"/>
<contactref element="D4" pad="A"/>
<contactref element="R7" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VDD">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="12"/>
<contactref element="C4" pad="+"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="Q1" pad="S"/>
<contactref element="R7" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="CON1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="CON1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="D3" pad="A"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="N$8">
</signal>
<signal name="N$19">
<contactref element="IC1" pad="4"/>
<contactref element="C6" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="9"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="NTC" pad="1"/>
<contactref element="D2" pad="C"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="N$25">
</signal>
<signal name="N$26">
</signal>
<signal name="N$27">
</signal>
<signal name="N$28">
</signal>
<signal name="N$29">
</signal>
<signal name="N$30">
</signal>
<signal name="N$31">
</signal>
<signal name="N$32">
</signal>
<signal name="N$2">
</signal>
<signal name="N$15">
<contactref element="L1" pad="2"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$12">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="N$22">
</signal>
<signal name="N$4">
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
