<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="75.87" y1="15.23" x2="75.87" y2="41.9" width="0" layer="20"/>
<wire x1="75.87" y1="41.9" x2="26.67" y2="41.9" width="0" layer="20"/>
<wire x1="26.67" y1="41.9" x2="26.67" y2="15.23" width="0" layer="20"/>
<wire x1="75.87" y1="15.23" x2="26.67" y2="15.23" width="0" layer="20"/>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="atmel">
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="1X03">
</package>
<package name="AXIAL-0.3">
</package>
<package name="1X02">
</package>
<package name="1X06">
</package>
<package name="1X04">
</package>
<package name="RESONATOR-PTH">
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="transistor-npn">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LONGPADS">
</package>
<package name="1X01">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="atmel" package="DIL28-3" value="MEGA8-P">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="R1" library="SparkFun" package="AXIAL-0.3" value="10K"/>
<element name="JP7" library="SparkFun" package="1X02" value="LED"/>
<element name="JP11" library="SparkFun" package="1X06" value="USB to Serial"/>
<element name="JP14" library="SparkFun" package="1X03" value="TurretA"/>
<element name="JP15" library="SparkFun" package="1X03" value="Turret B"/>
<element name="JP1" library="SparkFun" package="1X04" value="HBridge"/>
<element name="16MHZ" library="SparkFun" package="RESONATOR-PTH" value="RESONATORPTH"/>
<element name="Q3" library="transistor-npn" package="TO92" value="2N5088"/>
<element name="R6" library="SparkFun" package="AXIAL-0.3" value="1K"/>
<element name="JP2" library="SparkFun" package="1X04" value="HBridge"/>
<element name="JP3" library="SparkFun" package="1X04" value="Unused"/>
<element name="JP4" library="SparkFun" package="1X03" value="Servo"/>
<element name="JP6" library="SparkFun" package="1X02" value="LED"/>
<element name="U$1" library="SparkFun" package="STAND-OFF" value=""/>
<element name="U$3" library="SparkFun" package="STAND-OFF" value=""/>
<element name="U$4" library="SparkFun" package="STAND-OFF" value=""/>
<element name="JP8" library="SparkFun-Connectors" package="1X06_LONGPADS" value=""/>
<element name="JP5" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="JP9" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="JP10" library="SparkFun-Connectors" package="1X01" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="22"/>
<contactref element="IC1" pad="8"/>
<contactref element="JP14" pad="2"/>
<contactref element="JP7" pad="1"/>
<contactref element="JP11" pad="6"/>
<contactref element="16MHZ" pad="2"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP8" pad="3"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="20"/>
<contactref element="JP14" pad="1"/>
<contactref element="JP7" pad="2"/>
<contactref element="JP11" pad="3"/>
<contactref element="R1" pad="P$1"/>
<contactref element="Q3" pad="1"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP6" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP10" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="25"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="26"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="D8">
<contactref element="IC1" pad="14"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="D10">
<contactref element="IC1" pad="16"/>
<contactref element="JP8" pad="6"/>
</signal>
<signal name="D12">
<contactref element="IC1" pad="18"/>
</signal>
<signal name="3.3V">
<contactref element="JP11" pad="2"/>
</signal>
<signal name="D9">
<contactref element="IC1" pad="15"/>
<contactref element="JP8" pad="5"/>
</signal>
<signal name="D11">
<contactref element="IC1" pad="17"/>
</signal>
<signal name="D13">
<contactref element="IC1" pad="19"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="D3">
<contactref element="IC1" pad="5"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="D4">
<contactref element="IC1" pad="6"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="D2">
<contactref element="IC1" pad="4"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="D7">
<contactref element="IC1" pad="13"/>
<contactref element="JP15" pad="3"/>
</signal>
<signal name="D1">
<contactref element="IC1" pad="3"/>
<contactref element="JP11" pad="4"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="D0">
<contactref element="IC1" pad="2"/>
<contactref element="JP11" pad="5"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="JP11" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="D18">
<contactref element="IC1" pad="27"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="D14">
<contactref element="IC1" pad="23"/>
<contactref element="JP15" pad="2"/>
</signal>
<signal name="D15">
<contactref element="IC1" pad="24"/>
<contactref element="JP15" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="10"/>
<contactref element="16MHZ" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="9"/>
<contactref element="16MHZ" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="Q3" pad="2"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="IROUT">
<contactref element="JP14" pad="3"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="D19">
<contactref element="IC1" pad="28"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="D5">
<contactref element="IC1" pad="11"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="D6">
<contactref element="IC1" pad="12"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="JP8" pad="4"/>
<contactref element="JP5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
