;      This program is free software: you can redistribute it and/or modify
;    it under the terms of the GNU General Public License as published by
;    the Free Software Foundation, either version 3 of the License, or
;    (at your option) any later version.

;    This program is distributed in the hope that it will be useful,
;    but WITHOUT ANY WARRANTY; without even the implied warranty of
;    MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
;    GNU General Public License for more details.
;
;    You should have received a copy of the GNU General Public License
;    along with this program.  If not, see <http://www.gnu.org/licenses/>.

; This may be used for personal use, no commercial use is allowed without permission.


; Updated February 15, 2012

;=============     www.ChromationSystems.com       ============

; ==============   For Kits, Projects, Parts        ============

; == Please Support Future Projects by Visiting the Store or Donating ==


Usage: 

Press button quickly to change mode between fade and select.

Press and hold to Dim 100% - 50%

When in Dim Mode, quickly press to exit dim selection and return to
color select or speed select


Changes v.1 to v.2

- Faster PWM Rate
- Better Dimming down to 50%
- Color Select now goes Red -> Green -> Blue -> White (added white)
- Refined user controls
- Fixed misc bugs


Supplied in this zip are 

- Schematics
- PCB Copper layout
- PCB Silkscreen layer
- HEX File for PIC12F675 - regular version
- HEX File for mod 1
- HEX File for mod 2
- Datasheet v.1

Please help support this and future projects by Buying a Kit or PCB from my Store, or Donating

FUSES:

_CP_OFF & _CPD_OFF & _BODEN_OFF & _MCLRE_OFF & _WDT_OFF & _PWRTE_ON & _INTRC_OSC_NOCLKOUT  
