<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="65.71" y2="0" width="0" layer="20"/>
<wire x1="65.71" y1="0" x2="65.71" y2="30.47" width="0" layer="20"/>
<wire x1="65.71" y1="30.47" x2="0" y2="30.47" width="0" layer="20"/>
<wire x1="0" y1="30.47" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="cap-pan40">
<description>&lt;b&gt;Panasonic Electrolytic, Film and Tantalum Capacitors&lt;/b&gt;&lt;br&gt;

&lt;h4&gt;&lt;i&gt;Created by Bob Starr (rtzaudio@mindspring.com)&lt;br&gt;
Updated 01/08/2005&lt;/i&gt;&lt;/h4&gt;

&lt;p&gt;&lt;b&gt;The following Panasonic capactor types are supported by this library:&lt;/b&gt;
&lt;p&gt;M/NHG/FC/EB/KS/KG/TS/AA Series Radial Electrolytics&lt;br&gt;
  B/V/E/F Series Polyester Film&lt;br&gt;
  EF Series Tantalum Capacitors&lt;br&gt;
  CD/FD/H/S/UD/UE Series SMD Electrolytics&lt;br&gt;
  VV/TA/HD/VA/VS/HA/HB/FC/FK/EB SMD Electrolytics&lt;br&gt;&lt;br&gt;
 NOTE: All parts use .0125" grid spacing except where noted.&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All capacitors are grouped by the following naming conventions:&lt;/h4&gt;&lt;/p&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C-BP&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C-CA&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C-NP&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C-PA&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Axial Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C-PR&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;
&lt;small&gt;&lt;i&gt;Copyright (C) 2004, Bob Starr&lt;/i&gt;&lt;/small&gt;</description>
<packages>
<package name="E5,0-10">
<description>&lt;b&gt;POLCAP RADIAL&lt;/b&gt;&lt;p&gt;
5.0 mm lead spacing, 10 mm diameter, grid 0.0125 inch</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DO-1N4148">
</package>
<package name="1X01-CLEANBIG">
</package>
<package name="FEATHERWING_DIM">
</package>
</packages>
</library>
<library name="ubloxLib">
<packages>
<package name="MAX-M8">
<description>u-blox MAX GNSS module</description>
</package>
</packages>
</library>
<library name="diy-modules">
<description>&lt;b&gt;DIY Modules for Arduino, Raspberry Pi, CubieBoard etc.&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
The library contains a list of symbols and footprints for popular, cheap and easy-to-use electronic modules.&lt;br&gt;
The modules are intend to work with microprocessor-based platforms such as &lt;a href="http://arduino.cc"&gt;Arduino&lt;/a&gt;, &lt;a href="http://raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt;, &lt;a href="http://cubieboard.org/"&gt;CubieBoard&lt;/a&gt;, &lt;a href="http://beagleboard.org/"&gt;BeagleBone&lt;/a&gt; and many others. There are many manufacturers of the modules in the world. Almost all of them can be bought on &lt;a href="ebay.com"&gt;ebay.com&lt;/a&gt;.&lt;br&gt;
&lt;br&gt;
By using this library, you can design a PCB for devices created with usage of modules. Even if you do not need to create PCB design, you can also use the library to quickly document your work by drawing schematics of devices built by you.&lt;br&gt;
&lt;br&gt;
The latest version, examples, photos and much more can be found at: &lt;b&gt;&lt;a href="http://diymodules.org/eagle"&gt;diymodules.org/eagle&lt;/a&gt;&lt;/b&gt;&lt;br&gt;&lt;br&gt;
Comments, suggestions and bug reports please send to: &lt;b&gt;&lt;a href="mailto:eagle@diymodules.org"&gt;eagle@diymodules.org&lt;/b&gt;&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Version: 1.8.0 (2017-Jul-02)&lt;/i&gt;&lt;br&gt;
&lt;i&gt;Created by: Miroslaw Brudnowski&lt;/i&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Released under the Creative Commons Attribution 4.0 International License: &lt;a href="http://creativecommons.org/licenses/by/4.0"&gt;http://creativecommons.org/licenses/by/4.0&lt;/a&gt;&lt;/i&gt;
&lt;br&gt;&lt;br&gt;
&lt;center&gt;
&lt;a href="http://diymodules.org/eagle"&gt;&lt;img src="http://www.diymodules.org/img/diymodules-lbr-image.php?v=1.8.0" alt="DIYmodules.org"&gt;&lt;/a&gt;
&lt;/center&gt;</description>
<packages>
<package name="TEMP-HUM-PRES-BME280">
<description>&lt;b&gt;Digital Humidity-Temperature-Pressure Sensor&lt;/b&gt; based on &lt;b&gt;BME280&lt;/b&gt; device</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C4" library="cap-pan40" package="E5,0-10" value=""/>
<element name="C5" library="cap-pan40" package="E5,0-10" value=""/>
<element name="D1" library="adafruit" package="DO-1N4148" value=""/>
<element name="GND" library="adafruit" package="1X01-CLEANBIG" value=""/>
<element name="GPS_ANT" library="adafruit" package="1X01-CLEANBIG" value=""/>
<element name="MS2" library="adafruit" package="FEATHERWING_DIM" value="FEATHERWING_NODIM"/>
<element name="U$1" library="ubloxLib" package="MAX-M8" value="MAX-M8"/>
<element name="VCC" library="adafruit" package="1X01-CLEANBIG" value=""/>
<element name="BME280" library="diy-modules" package="TEMP-HUM-PRES-BME280" value="TEMP-HUM-PRES-BME280"/>
</elements>
<signals>
<signal name="9_V_RESET_N">
<contactref element="U$1" pad="9_RESET_N"/>
</signal>
<signal name="SDI/SDA">
<contactref element="MS2" pad="17"/>
<contactref element="BME280" pad="4"/>
</signal>
<signal name="SCK/SCL">
<contactref element="MS2" pad="18"/>
<contactref element="BME280" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="GPS_ANT" pad="1"/>
<contactref element="U$1" pad="11_RF_IN"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="2_TXD"/>
<contactref element="MS2" pad="14"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="3_RXD"/>
<contactref element="MS2" pad="15"/>
</signal>
<signal name="N$6">
<contactref element="GND" pad="1"/>
<contactref element="U$1" pad="10_GND"/>
<contactref element="U$1" pad="12_GND"/>
<contactref element="U$1" pad="1_GND"/>
<contactref element="MS2" pad="4"/>
<contactref element="C4" pad="-"/>
<contactref element="BME280" pad="2"/>
</signal>
<signal name="3V">
<contactref element="U$1" pad="6_V_BCKP"/>
<contactref element="U$1" pad="8_VCC"/>
<contactref element="U$1" pad="7_VCC_IO"/>
<contactref element="MS2" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="C5" pad="+"/>
<contactref element="BME280" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="A"/>
<contactref element="VCC" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="C4" pad="+"/>
<contactref element="C5" pad="-"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
