____doifc
___boot_delay128k
___boot_delay12k
___boot_delay16k
___boot_delay24k
___boot_delay32k
___boot_delay48k
___boot_delay4k
___boot_delay64k
___boot_delay8k
__ca2aw
__cc2d
__cc2dw
__cca2aw
__ccs2s
__cs2s
__flash_size
__fzins
__low_savebsr
__low_savestatus
__low_savewreg
_c1out
_c2out
_ccp1
_ccp1_p1a
_ccp2
_ccp2_p2a
_ck2
_dat
_dt2
_flt0
_input
_int1
_int2
_int3
_null
_output
_p1b
_p1c
_p1d
_p2b
_p2c
_p2d
_rx2_dt2
_sck2
_sck2in
_sdi2
_sdo2
_ss2in
_ssdma
_t0cki
_t1g
_t3cki
_t3g
_tx2_ck2
_ulpout
a
abden
abden_baudcon_bit
abden_bit
abdovf
abdovf_baudcon_bit
abdovf_bit
access
ackdt
ackdt_bit
ackdt_ssp1con2_bit
acken
acken_bit
acken_ssp1con2_bit
ackstat
ackstat_bit
ackstat_ssp1con2_bit
acqt0
acqt0_bit
acqt1
acqt1_bit
acqt2
acqt2_bit
acss
acss_bit
actvie
actvie_bit
actvif
actvif_bit
adcal
adcal_bit
adcon0
adcon1
adcs0
adcs0_bit
adcs1
adcs1_bit
adcs2
adcs2_bit
add_32x32_fp
adden
adden_bit
adden_rcsta_bit
adden1
adden1_bit
adden2
adden2_bit
addr0
addr0_bit
addr1
addr1_bit
addr2
addr2_bit
addr3
addr3_bit
addr4
addr4_bit
addr5
addr5_bit
addr6
addr6_bit
aden
aden_bit
adfm
adfm_bit
adie
adie_bit
adif
adif_bit
adip
adip_bit
admsk1
admsk1_bit
admsk1_ssp1con2_bit
admsk2
admsk2_bit
admsk2_ssp1con2_bit
admsk3
admsk3_bit
admsk3_ssp1con2_bit
admsk4
admsk4_bit
admsk4_ssp1con2_bit
admsk5
admsk5_bit
admsk5_ssp1con2_bit
adon
adon_bit
adres
adresh
adresl
alrmcfg
alrmen
alrmen_bit
alrmptr0
alrmptr0_bit
alrmptr1
alrmptr1_bit
alrmrpt
alrmvalh
alrmvall
amask0
amask0_bit
amask1
amask1_bit
amask2
amask2_bit
amask3
amask3_bit
an0
an0_bit
an1
an1_bit
an10
an10_bit
an11
an11_bit
an12
an12_bit
an2
an2_bit
an3
an3_bit
an4
an4_bit
an8
an8_bit
an9
an9_bit
ancon0
ancon1
arpt0
arpt0_bit
arpt1
arpt1_bit
arpt2
arpt2_bit
arpt3
arpt3_bit
arpt4
arpt4_bit
arpt5
arpt5_bit
arpt6
arpt6_bit
arpt7
arpt7_bit
b0
b1
b2
b3
b4
b5
b6
b7
banked
baudcon
baudcon1
baudcon2
baudctl
bcd2dec
bcd2dec16
bcddevice
bcdusb
bcl1ie
bcl1ie_bit
bcl1if
bcl1if_bit
bcl1ip
bcl1ip_bit
bcl2ie
bcl2ie_bit
bcl2if
bcl2if_bit
bcl2ip
bcl2ip_bit
bclie
bclie_bit
bclif
bclif_bit
bclip
bclip_bit
bdescriptortype
bdeviceclass
bdeviceprotocol
bdevicesubclass
bdsctype
bdsctype
bdsctype
bf
bf_bit
bf_ssp1stat_bit
bf1
bf1_bit
bgvst
bgvst_bit
blength
blength
blength
blength
bmaxpacketsize0
bnumconfigurations
bor
bor_bit
brg16
brg16_baudcon_bit
brg16_bit
brgh
brgh_bit
brgh_txsta_bit
brgh1
brgh1_bit
brgh2
brgh2_bit
bsr
btoee
btoee_bit
btoef
btoef_bit
btsee
btsee_bit
btsef
btsef_bit
byte2double
bytetohex
bytetostr
c
c_bit
c1ina
c1ina_bit
c1inb
c1inb_bit
c2ina
c2ina_bit
c2inb
c2inb_bit
cal0
cal0_bit
cal1
cal1_bit
cal2
cal2_bit
cal3
cal3_bit
cal4
cal4_bit
cal5
cal5_bit
cal6
cal6_bit
cal7
cal7_bit
cch0
cch0_bit
cch0_cm1con_bit
cch0_cm1con1_bit
cch0_cm2con1_bit
cch01
cch01_bit
cch01_cm1con1_bit
cch1
cch1_bit
cch1_cm1con_bit
cch1_cm1con1_bit
cch1_cm2con1_bit
cch11
cch11_bit
cch11_cm1con1_bit
ccp1con
ccp1ie
ccp1ie_bit
ccp1if
ccp1if_bit
ccp1ip
ccp1ip_bit
ccp1m0
ccp1m0_bit
ccp1m1
ccp1m1_bit
ccp1m2
ccp1m2_bit
ccp1m3
ccp1m3_bit
ccp1x
ccp1x_bit
ccp1y
ccp1y_bit
ccp2con
ccp2ie
ccp2ie_bit
ccp2if
ccp2if_bit
ccp2ip
ccp2ip_bit
ccp2m0
ccp2m0_bit
ccp2m1
ccp2m1_bit
ccp2m2
ccp2m2_bit
ccp2m3
ccp2m3_bit
ccp2x
ccp2x_bit
ccp2y
ccp2y_bit
ccpr1
ccpr1h
ccpr1l
ccpr2
ccpr2h
ccpr2l
chime
chime_bit
chs0
chs0_bit
chs1
chs1_bit
chs2
chs2_bit
chs3
chs3_bit
ck1
ck1_bit
ck20
ck20_bit
ck21
ck21_bit
ck22
ck22_bit
ck23
ck23_bit
ck24
ck24_bit
cke
cke_bit
cke_ssp1stat_bit
cke1
cke1_bit
ckp
ckp_bit
ckp_ssp1con1_bit
ckp1
ckp1_bit
clki
clki_bit
clko
clko_bit
cm
cm_bit
cm1con
cm1con1
cm1ie
cm1ie_bit
cm1if
cm1if_bit
cm1ip
cm1ip_bit
cm2con
cm2con1
cm2ie
cm2ie_bit
cm2if
cm2if_bit
cm2ip
cm2ip_bit
cmpl0
cmpl0_bit
cmpl0_pstr1con_bit
cmpl1
cmpl1_bit
cmpl1_pstr1con_bit
cmstat
cmstatus
coe
coe_bit
coe_cm1con_bit
coe_cm1con1_bit
coe_cm2con1_bit
coe1
coe1_bit
coe1_cm1con1_bit
comfrem
compare_double
con
con_bit
con_cm1con_bit
con_cm1con1_bit
con_cm2con1_bit
con1
con1_bit
con1_cm1con1_bit
configdescriptor1
cout1
cout1_bit
cout2
cout2_bit
cpol
cpol_bit
cpol_cm1con_bit
cpol_cm1con1_bit
cpol_cm2con1_bit
cpol1
cpol1_bit
cpol1_cm1con1_bit
crc16ee
crc16ee_bit
crc16ef
crc16ef_bit
crc5ee
crc5ee_bit
crc5ef
crc5ef_bit
cref
cref_bit
cref_cm1con_bit
cref_cm1con1_bit
cref_cm2con1_bit
cref1
cref1_bit
cref1_cm1con1_bit
cren
cren_bit
cren_rcsta_bit
cren1
cren1_bit
cren2
cren2_bit
csrc
csrc_bit
csrc_txsta_bit
csrc1
csrc1_bit
csrc2
csrc2_bit
ctedg1
ctedg1_bit
ctedg2
ctedg2_bit
ctmuconh
ctmuconl
ctmuen
ctmuen_bit
ctmuicon
ctmuie
ctmuie_bit
ctmuif
ctmuif_bit
ctmuip
ctmuip_bit
ctmusidl
ctmusidl_bit
ctpls
ctpls_bit
cttrig
cttrig_bit
cvr0
cvr0_bit
cvr1
cvr1_bit
cvr2
cvr2_bit
cvr3
cvr3_bit
cvrcon
cvref_minus
cvref_minus_bit
cvren
cvren_bit
cvroe
cvroe_bit
cvrr
cvrr_bit
cvrss
cvrss_bit
d
d_a
d_a_bit
d_a1
d_a1_bit
d_bit
d_minus
d_minus_bit
d_not_a
d_not_a_bit
d_not_a_ssp1stat_bit
d_not_a1
d_not_a1_bit
d_plus
d_plus_bit
d1
d1_bit
data_address
data_address_bit
data_address1
data_address1_bit
dc
dc_bit
dc1b0
dc1b0_bit
dc1b1
dc1b1_bit
dc2b0
dc2b0_bit
dc2b1
dc2b1_bit
dec2bcd
dec2bcd16
delay_100ms
delay_10ms
delay_10us
delay_1ms
delay_1sec
delay_1us
delay_22us
delay_500us
delay_50us
delay_5500us
delay_5ms
delay_80us
delay_8ms
delay_cyc
device_dsc
dfn8ee
dfn8ee_bit
dfn8ef
dfn8ef_bit
dir_
dir__bit
div_16x16_s
div_16x16_s_l
div_16x16_u
div_32x32_fp
div_32x32_s
div_32x32_u
div_8x8_s
div_8x8_u
dlycyc0
dlycyc0_bit
dlycyc1
dlycyc1_bit
dlycyc2
dlycyc2_bit
dlycyc3
dlycyc3_bit
dlyinten
dlyinten_bit
dmabch
dmabcl
dmacnthb0
dmacnthb0_bit
dmacnthb1
dmacnthb1_bit
dmacon1
dmacon2
dmaen
dmaen_bit
dmarcptrhb0
dmarcptrhb0_bit
dmarcptrhb1
dmarcptrhb1_bit
dmarcptrhb2
dmarcptrhb2_bit
dmarcptrhb3
dmarcptrhb3_bit
dmatxptrhb0
dmatxptrhb0_bit
dmatxptrhb1
dmatxptrhb1_bit
dmatxptrhb2
dmatxptrhb2_bit
dmatxptrhb3
dmatxptrhb3_bit
done
done_bit
double2byte
double2int
double2longint
double2longword
double2word
ds
ds_bit
dsbor
dsbor_bit
dsconh
dsconl
dsen
dsen_bit
dsflt
dsflt_bit
dsgpr0
dsgpr1
dsint0
dsint0_bit
dsmclr
dsmclr_bit
dspor
dspor_bit
dsrtc
dsrtc_bit
dsulp
dsulp_bit
dsulpen
dsulpen_bit
dswakeh
dswakel
dswdt
dswdt_bit
dt1
dt1_bit
duplex0
duplex0_bit
duplex1
duplex1_bit
eccp1as
eccp1as0
eccp1as0_bit
eccp1as1
eccp1as1_bit
eccp1as2
eccp1as2_bit
eccp1ase
eccp1ase_bit
eccp1con
eccp1del
eccp1od
eccp1od_bit
eccp2as
eccp2as0
eccp2as0_bit
eccp2as1
eccp2as1_bit
eccp2as2
eccp2as2_bit
eccp2ase
eccp2ase_bit
eccp2con
eccp2del
eccp2od
eccp2od_bit
edg1pol
edg1pol_bit
edg1sel0
edg1sel0_bit
edg1sel1
edg1sel1_bit
edg1stat
edg1stat_bit
edg2pol
edg2pol_bit
edg2sel0
edg2sel0_bit
edg2sel1
edg2sel1_bit
edg2stat
edg2stat_bit
edgen
edgen_bit
edgseqen
edgseqen_bit
eecon1
eecon2
endp0
endp0_bit
endp1
endp1_bit
endp2
endp2_bit
endp3
endp3_bit
ep_in_interval
ep_out_interval
epcondis
epcondis_bit
epcondis_uep1_bit
epcondis_uep10_bit
epcondis_uep11_bit
epcondis_uep12_bit
epcondis_uep13_bit
epcondis_uep14_bit
epcondis_uep15_bit
epcondis_uep2_bit
epcondis_uep3_bit
epcondis_uep4_bit
epcondis_uep5_bit
epcondis_uep6_bit
epcondis_uep7_bit
epcondis_uep8_bit
epcondis_uep9_bit
ephshk
ephshk_bit
ephshk_uep1_bit
ephshk_uep10_bit
ephshk_uep11_bit
ephshk_uep12_bit
ephshk_uep13_bit
ephshk_uep14_bit
ephshk_uep15_bit
ephshk_uep2_bit
ephshk_uep3_bit
ephshk_uep4_bit
ephshk_uep5_bit
ephshk_uep6_bit
ephshk_uep7_bit
ephshk_uep8_bit
ephshk_uep9_bit
epinen
epinen_bit
epinen_uep1_bit
epinen_uep10_bit
epinen_uep11_bit
epinen_uep12_bit
epinen_uep13_bit
epinen_uep14_bit
epinen_uep15_bit
epinen_uep2_bit
epinen_uep3_bit
epinen_uep4_bit
epinen_uep5_bit
epinen_uep6_bit
epinen_uep7_bit
epinen_uep8_bit
epinen_uep9_bit
epouten
epouten_bit
epouten_uep1_bit
epouten_uep10_bit
epouten_uep11_bit
epouten_uep12_bit
epouten_uep13_bit
epouten_uep14_bit
epouten_uep15_bit
epouten_uep2_bit
epouten_uep3_bit
epouten_uep4_bit
epouten_uep5_bit
epouten_uep6_bit
epouten_uep7_bit
epouten_uep8_bit
epouten_uep9_bit
epstall
epstall_bit
epstall_uep1_bit
epstall_uep10_bit
epstall_uep11_bit
epstall_uep12_bit
epstall_uep13_bit
epstall_uep14_bit
epstall_uep15_bit
epstall_uep2_bit
epstall_uep3_bit
epstall_uep4_bit
epstall_uep5_bit
epstall_uep6_bit
epstall_uep7_bit
epstall_uep8_bit
epstall_uep9_bit
equals_double
evpol0
evpol0_bit
evpol0_cm1con_bit
evpol0_cm1con1_bit
evpol0_cm2con1_bit
evpol01
evpol01_bit
evpol01_cm1con1_bit
evpol1
evpol1_bit
evpol1_cm1con_bit
evpol1_cm1con1_bit
evpol1_cm2con1_bit
evpol11
evpol11_bit
evpol11_cm1con1_bit
f
fast
ferr
ferr_bit
ferr_rcsta_bit
ferr1
ferr1_bit
ferr2
ferr2_bit
fixsign32
floattostr
flt00
flt00_bit
flt01
flt01_bit
flt02
flt02_bit
flt03
flt03_bit
flt04
flt04_bit
free
free_bit
frm0
frm0_bit
frm1
frm1_bit
frm10
frm10_bit
frm2
frm2_bit
frm3
frm3_bit
frm4
frm4_bit
frm5
frm5_bit
frm6
frm6_bit
frm7
frm7_bit
frm8
frm8_bit
frm9
frm9_bit
fsen
fsen_bit
fsr0
fsr0h
fsr0l
fsr0ptr
fsr1
fsr1h
fsr1l
fsr1ptr
fsr2
fsr2h
fsr2l
fsr2ptr
gcen
gcen_bit
gcen_ssp1con2_bit
gen_enable
gen_read
gen_write
get_fosc_khz
get_mark
get_nec_byte
get_space
gie
gie_bit
gie_gieh
gie_gieh_bit
gieh
gieh_bit
giel
giel_bit
go
go_bit
go_done
go_done_bit
go_not_done
go_not_done_bit
halfsec
halfsec_bit
hid_disable
hid_enable
hid_input_report_bytes
hid_output_report_bytes
hid_read
hid_rpt_desc
hid_write
hlvdcon
hlvden
hlvden_bit
hlvdin
hlvdin_bit
hlvdl0
hlvdl0_bit
hlvdl1
hlvdl1_bit
hlvdl2
hlvdl2_bit
hlvdl3
hlvdl3_bit
i2c_dat
i2c_dat_bit
i2c_dat1
i2c_dat1_bit
i2c_read
i2c_read_bit
i2c_read1
i2c_read1_bit
i2c_start_
i2c_start__bit
i2c_start1
i2c_start1_bit
i2c_stop_
i2c_stop__bit
i2c_stop1
i2c_stop1_bit
ic10
ic10_bit
ic11
ic11_bit
ic12
ic12_bit
ic13
ic13_bit
ic14
ic14_bit
ic20
ic20_bit
ic21
ic21_bit
ic22
ic22_bit
ic23
ic23_bit
ic24
ic24_bit
ics_auto
ics_off
id
idissen
idissen_bit
idleie
idleie_bit
idleif
idleif_bit
idlen
idlen_bit
idproduct
idvendor
imanufacturer
indf0
indf1
indf2
int0
int0_bit
int0e
int0e_bit
int0f
int0f_bit
int0ie
int0ie_bit
int0if
int0if_bit
int10
int10_bit
int11
int11_bit
int12
int12_bit
int13
int13_bit
int14
int14_bit
int1e
int1e_bit
int1f
int1f_bit
int1ie
int1ie_bit
int1if
int1if_bit
int1ip
int1ip_bit
int1p
int1p_bit
int20
int20_bit
int21
int21_bit
int22
int22_bit
int23
int23_bit
int24
int24_bit
int2double
int2e
int2e_bit
int2f
int2f_bit
int2ie
int2ie_bit
int2if
int2if_bit
int2ip
int2ip_bit
int2p
int2p_bit
int30
int30_bit
int31
int31_bit
int32
int32_bit
int33
int33_bit
int34
int34_bit
int3e
int3e_bit
int3f
int3f_bit
int3ie
int3ie_bit
int3if
int3if_bit
int3ip
int3ip_bit
int3p
int3p_bit
intcon
intcon2
intcon3
intedg0
intedg0_bit
intedg1
intedg1_bit
intedg2
intedg2_bit
intedg3
intedg3_bit
interrupt
intlvl0
intlvl0_bit
intlvl1
intlvl1_bit
intlvl2
intlvl2_bit
intlvl3
intlvl3_bit
intsrc
intsrc_bit
inttohex
inttostr
inttostrwithzeros
iolock
iolock_bit
ipen
ipen_bit
ipr1
ipr2
ipr3
iproduct
ir_in
ir_in_direction
ir_result
ircf0
ircf0_bit
ircf1
ircf1_bit
ircf2
ircf2_bit
irng0
irng0_bit
irng1
irng1_bit
irvst
irvst_bit
isalnum
isalpha
iscntrl
isdigit
iserialnumber
isgraph
islower
ispunct
isspace
isupper
isxdigit
itrim0
itrim0_bit
itrim1
itrim1_bit
itrim2
itrim2_bit
itrim3
itrim3_bit
itrim4
itrim4_bit
itrim5
itrim5_bit
kbi0
kbi0_bit
kbi1
kbi1_bit
kbi2
kbi2_bit
kbi3
kbi3_bit
key
lata
lata0
lata0_bit
lata1
lata1_bit
lata2
lata2_bit
lata3
lata3_bit
lata5
lata5_bit
lata6
lata6_bit
lata7
lata7_bit
latb
latb0
latb0_bit
latb1
latb1_bit
latb2
latb2_bit
latb3
latb3_bit
latb4
latb4_bit
latb5
latb5_bit
latb6
latb6_bit
latb7
latb7_bit
latc
latc0
latc0_bit
latc1
latc1_bit
latc2
latc2_bit
latc4
latc4_bit
latc5
latc5_bit
latc6
latc6_bit
latc7
latc7_bit
lock_iolock
longint2double
longinttohex
longinttostrwithzeros
longjmp
longtostr
longword2double
longwordtohex
longwordtostr
longwordtostrwithzeros
ltrim
lvdie
lvdie_bit
lvdif
lvdif_bit
lvdip
lvdip_bit
lvdstat
lvdstat_bit
main
memchr
memcmp
memcpy
memmove
memset
modifier
msk0
msk0_bit
msk0_ssp1add_bit
msk01
msk01_bit
msk1
msk1_bit
msk1_ssp1add_bit
msk11
msk11_bit
msk2
msk2_bit
msk2_ssp1add_bit
msk21
msk21_bit
msk3
msk3_bit
msk3_ssp1add_bit
msk31
msk31_bit
msk4
msk4_bit
msk4_ssp1add_bit
msk41
msk41_bit
msk5
msk5_bit
msk5_ssp1add_bit
msk51
msk51_bit
msk6
msk6_bit
msk6_ssp1add_bit
msk61
msk61_bit
msk7
msk7_bit
msk7_ssp1add_bit
msk71
msk71_bit
mul_16x16_s
mul_16x16_u
mul_32x32_fp
mul_32x32_s
mul_32x32_u
mul_8x8_s
n
n_bit
nec_read
not_a
not_a_bit
not_a1
not_a1_bit
not_address
not_address_bit
not_address1
not_address1_bit
not_bor
not_bor_bit
not_cm
not_cm_bit
not_done
not_done_bit
not_pd
not_pd_bit
not_por
not_por_bit
not_rbpu
not_rbpu_bit
not_rc8
not_rc8_bit
not_ri
not_ri_bit
not_ss1
not_ss1_bit
not_to
not_to_bit
not_tx8
not_tx8_bit
not_uoe
not_uoe_bit
not_w
not_w_bit
not_w1
not_w1_bit
not_write
not_write_bit
not_write1
not_write1_bit
nrm3232
nrm4032
odcon1
odcon2
odcon3
oerr
oerr_bit
oerr_rcsta_bit
oerr1
oerr1_bit
oerr2
oerr2_bit
osc1
osc1_bit
osc2
osc2_bit
osccon
oscfie
oscfie_bit
oscfif
oscfif_bit
oscfip
oscfip_bit
osctune
osts
osts_bit
ov
ov_bit
p
p_bit
p_ssp1stat_bit
p1
p1_bit
p1dc0
p1dc0_bit
p1dc1
p1dc1_bit
p1dc2
p1dc2_bit
p1dc3
p1dc3_bit
p1dc4
p1dc4_bit
p1dc5
p1dc5_bit
p1dc6
p1dc6_bit
p1m0
p1m0_bit
p1m1
p1m1_bit
p1rsen
p1rsen_bit
p2dc0
p2dc0_bit
p2dc0_pstr2con_bit
p2dc1
p2dc1_bit
p2dc1_pstr2con_bit
p2dc2
p2dc2_bit
p2dc2_pstr2con_bit
p2dc3
p2dc3_bit
p2dc3_pstr2con_bit
p2dc4
p2dc4_bit
p2dc4_pstr2con_bit
p2dc5
p2dc5_bit
p2dc5_pstr2con_bit
p2dc6
p2dc6_bit
p2dc6_pstr2con_bit
p2m0
p2m0_bit
p2m1
p2m1_bit
p2rsen
p2rsen_bit
padcfg1
pc
pcfg0
pcfg0_bit
pcfg1
pcfg1_bit
pcfg10
pcfg10_bit
pcfg11
pcfg11_bit
pcfg12
pcfg12_bit
pcfg2
pcfg2_bit
pcfg3
pcfg3_bit
pcfg4
pcfg4_bit
pcfg8
pcfg8_bit
pcfg9
pcfg9_bit
pcl
pclath
pclatu
pcu0
pcu0_bit
pcu1
pcu1_bit
pcu2
pcu2_bit
pcu3
pcu3_bit
pcu4
pcu4_bit
pd
pd_bit
peie
peie_bit
peie_giel
peie_giel_bit
pen
pen_bit
pen_ssp1con2_bit
pgc
pgc_bit
pgd
pgd_bit
pidee
pidee_bit
pidef
pidef_bit
pie1
pie2
pie3
pir1
pir2
pir3
pktdis
pktdis_bit
pllen
pllen_bit
plusw0
plusw1
plusw2
pmpttl
pmpttl_bit
por
por_bit
porta
portb
portc
postdec0
postdec1
postdec2
postinc0
postinc1
postinc2
ppb0
ppb0_bit
ppb1
ppb1_bit
ppbi
ppbi_bit
ppbrst
ppbrst_bit
pps_mapping
pps_mapping_nolock
ppscon
pr2
pr4
preinc0
preinc1
preinc2
prod
prodh
prodl
psa
psa_bit
pss1ac0
pss1ac0_bit
pss1ac1
pss1ac1_bit
pss1bd0
pss1bd0_bit
pss1bd1
pss1bd1_bit
pss2ac0
pss2ac0_bit
pss2ac1
pss2ac1_bit
pss2bd0
pss2bd0_bit
pss2bd1
pss2bd1_bit
pstr1con
pstr2con
pwm1con
pwm2con
r
r_bit
r_not_w
r_not_w_bit
r_not_w_ssp1stat_bit
r_not_w1
r_not_w1_bit
r_w
r_w_bit
r_w1
r_w1_bit
r0
r1
r1_
r1__bit
r10
r11
r12
r13
r14
r15
r16
r17
r18
r19
r2
r20
r3
r4
r5
r6
r7
r8
r9
ra0
ra0_bit
ra1
ra1_bit
ra2
ra2_bit
ra3
ra3_bit
ra5
ra5_bit
ra6
ra6_bit
ra7
ra7_bit
rb0
rb0_bit
rb1
rb1_bit
rb2
rb2_bit
rb3
rb3_bit
rb4
rb4_bit
rb5
rb5_bit
rb6
rb6_bit
rb7
rb7_bit
rbie
rbie_bit
rbif
rbif_bit
rbip
rbip_bit
rbpu
rbpu_bit
rc0
rc0_bit
rc1
rc1_bit
rc1ie
rc1ie_bit
rc1if
rc1if_bit
rc1ip
rc1ip_bit
rc2
rc2_bit
rc2ie
rc2ie_bit
rc2if
rc2if_bit
rc2ip
rc2ip_bit
rc4
rc4_bit
rc5
rc5_bit
rc6
rc6_bit
rc7
rc7_bit
rc8_9
rc8_9_bit
rc9
rc9_bit
rcd8
rcd8_bit
rcen
rcen_bit
rcen_ssp1con2_bit
rcidl
rcidl_baudcon_bit
rcidl_bit
rcie
rcie_bit
rcif
rcif_bit
rcip
rcip_bit
rcon
rcreg
rcreg1
rcreg2
rcsta
rcsta1
rcsta2
rcv
rcv_bit
rd16
rd16_bit
rd16_t1con_bit
rd161
rd161_bit
read_write
read_write_bit
read_write1
read_write1_bit
readbuff
refo
refo_bit
refocon
regslp
regslp_bit
release
release_bit
repeat
report
res032
resume_
resume__bit
retint
ri
ri_bit
rodiv0
rodiv0_bit
rodiv1
rodiv1_bit
rodiv2
rodiv2_bit
rodiv3
rodiv3_bit
roon
roon_bit
rosel
rosel_bit
rosslp
rosslp_bit
rp0
rp0_bit
rp1
rp1_bit
rp10
rp10_bit
rp11
rp11_bit
rp12
rp12_bit
rp13
rp13_bit
rp17
rp17_bit
rp18
rp18_bit
rp2
rp2_bit
rp3
rp3_bit
rp4
rp4_bit
rp5
rp5_bit
rp6
rp6_bit
rp7
rp7_bit
rp8
rp8_bit
rp9
rp9_bit
rpinr1
rpinr12
rpinr13
rpinr16
rpinr17
rpinr2
rpinr21
rpinr22
rpinr23
rpinr24
rpinr3
rpinr4
rpinr6
rpinr7
rpinr8
rpor0
rpor0_
rpor0__bit
rpor0__rpor1_bit
rpor0__rpor10_bit
rpor0__rpor11_bit
rpor0__rpor12_bit
rpor0__rpor13_bit
rpor0__rpor17_bit
rpor0__rpor18_bit
rpor0__rpor2_bit
rpor0__rpor3_bit
rpor0__rpor4_bit
rpor0__rpor5_bit
rpor0__rpor6_bit
rpor0__rpor7_bit
rpor0__rpor8_bit
rpor0__rpor9_bit
rpor1
rpor1_
rpor1__bit
rpor1__rpor1_bit
rpor1__rpor10_bit
rpor1__rpor11_bit
rpor1__rpor12_bit
rpor1__rpor13_bit
rpor1__rpor17_bit
rpor1__rpor18_bit
rpor1__rpor2_bit
rpor1__rpor3_bit
rpor1__rpor4_bit
rpor1__rpor5_bit
rpor1__rpor6_bit
rpor1__rpor7_bit
rpor1__rpor8_bit
rpor1__rpor9_bit
rpor10
rpor11
rpor12
rpor13
rpor17
rpor18
rpor2
rpor2_
rpor2__bit
rpor2__rpor1_bit
rpor2__rpor10_bit
rpor2__rpor11_bit
rpor2__rpor12_bit
rpor2__rpor13_bit
rpor2__rpor17_bit
rpor2__rpor18_bit
rpor2__rpor2_bit
rpor2__rpor3_bit
rpor2__rpor4_bit
rpor2__rpor5_bit
rpor2__rpor6_bit
rpor2__rpor7_bit
rpor2__rpor8_bit
rpor2__rpor9_bit
rpor3
rpor3_
rpor3__bit
rpor3__rpor1_bit
rpor3__rpor10_bit
rpor3__rpor11_bit
rpor3__rpor12_bit
rpor3__rpor13_bit
rpor3__rpor17_bit
rpor3__rpor18_bit
rpor3__rpor2_bit
rpor3__rpor3_bit
rpor3__rpor4_bit
rpor3__rpor5_bit
rpor3__rpor6_bit
rpor3__rpor7_bit
rpor3__rpor8_bit
rpor3__rpor9_bit
rpor4
rpor4_
rpor4__bit
rpor4__rpor1_bit
rpor4__rpor10_bit
rpor4__rpor11_bit
rpor4__rpor12_bit
rpor4__rpor13_bit
rpor4__rpor17_bit
rpor4__rpor18_bit
rpor4__rpor2_bit
rpor4__rpor3_bit
rpor4__rpor4_bit
rpor4__rpor5_bit
rpor4__rpor6_bit
rpor4__rpor7_bit
rpor4__rpor8_bit
rpor4__rpor9_bit
rpor5
rpor6
rpor7
rpor8
rpor9
rsen
rsen_bit
rsen_ssp1con2_bit
rtcc
rtcc_bit
rtccal
rtccfg
rtccie
rtccie_bit
rtccif
rtccif_bit
rtccip
rtccip_bit
rtcen
rtcen_bit
rtcoe
rtcoe_bit
rtcptr0
rtcptr0_bit
rtcptr1
rtcptr1_bit
rtcsync
rtcsync_bit
rtcvalh
rtcvall
rtcwdis
rtcwdis_bit
rtcwren
rtcwren_bit
rtrim
rtsecsel0
rtsecsel0_bit
rtsecsel1
rtsecsel1_bit
rx1
rx1_bit
rx2dt20
rx2dt20_bit
rx2dt21
rx2dt21_bit
rx2dt22
rx2dt22_bit
rx2dt23
rx2dt23_bit
rx2dt24
rx2dt24_bit
rx9
rx9_bit
rx9_rcsta_bit
rx91
rx91_bit
rx92
rx92_bit
rx9d
rx9d_bit
rx9d_rcsta_bit
rx9d1
rx9d1_bit
rx9d2
rx9d2_bit
rxaddrh
rxaddrl
rxdtp
rxdtp_baudcon_bit
rxdtp_bit
rxinc
rxinc_bit
s
s_bit
s_ssp1stat_bit
s1
s1_bit
sck1
sck1_bit
sck20
sck20_bit
sck21
sck21_bit
sck22
sck22_bit
sck23
sck23_bit
sck24
sck24_bit
scl1
scl1_bit
scs0
scs0_bit
scs1
scs1_bit
sda1
sda1_bit
sdi1
sdi1_bit
sdi20
sdi20_bit
sdi21
sdi21_bit
sdi22
sdi22_bit
sdi23
sdi23_bit
sdi24
sdi24_bit
sdiv3232l
sdo1
sdo1_bit
se0
se0_bit
sen
sen_bit
sen_ssp1con2_bit
sendb
sendb_bit
sendb_txsta_bit
sendb1
sendb1_bit
sendb2
sendb2_bit
sendkeycode
sendkeycode_func
setfdz32
setfov32
setfun32
setiov3224
setjmp
shorttohex
shorttostr
smp
smp_bit
smp_ssp1stat_bit
smp1
smp1_bit
sofie
sofie_bit
sofif
sofif_bit
sp0
sp0_bit
sp1
sp1_bit
sp2
sp2_bit
sp3
sp3_bit
sp4
sp4_bit
spbrg
spbrg1
spbrg2
spbrgh
spbrgh1
spbrgh2
spen
spen_bit
spen_rcsta_bit
spen1
spen1_bit
spen2
spen2_bit
spi1od
spi1od_bit
spi2od
spi2od_bit
sren
sren_bit
sren_rcsta_bit
sren1
sren1_bit
sren2
sren2_bit
ss20
ss20_bit
ss21
ss21_bit
ss22
ss22_bit
ss23
ss23_bit
ss24
ss24_bit
sscon0
sscon0_bit
sscon1
sscon1_bit
ssp1add
ssp1buf
ssp1con1
ssp1con2
ssp1ie
ssp1ie_bit
ssp1if
ssp1if_bit
ssp1ip
ssp1ip_bit
ssp1stat
ssp2add
ssp2buf
ssp2con1
ssp2con2
ssp2ie
ssp2ie_bit
ssp2if
ssp2if_bit
ssp2ip
ssp2ip_bit
ssp2stat
sspadd
sspbuf
sspcon1
sspcon2
sspen
sspen_bit
sspen_ssp1con1_bit
sspen1
sspen1_bit
sspie
sspie_bit
sspif
sspif_bit
sspip
sspip_bit
sspm0
sspm0_bit
sspm0_ssp1con1_bit
sspm01
sspm01_bit
sspm1
sspm1_bit
sspm1_ssp1con1_bit
sspm11
sspm11_bit
sspm2
sspm2_bit
sspm2_ssp1con1_bit
sspm21
sspm21_bit
sspm3
sspm3_bit
sspm3_ssp1con1_bit
sspm31
sspm31_bit
sspov
sspov_bit
sspov_ssp1con1_bit
sspov1
sspov1_bit
sspstat
stallie
stallie_bit
stallif
stallif_bit
status
stkful
stkful_bit
stkovf
stkovf_bit
stkptr
stkunf
stkunf_bit
stra
stra_bit
stra_pstr1con_bit
strb
strb_bit
strb_pstr1con_bit
strc
strc_bit
strc_pstr1con_bit
strcat
strchr
strcmp
strcpy
strcspn
strd
strd_bit
strd_pstr1con_bit
strd1
strd2
strd3
string
string
string
strlen
strncat
strncmp
strncpy
strpbrk
strrchr
strspn
strstr
strsync
strsync_bit
strsync_pstr1con_bit
strtok
sub_32x32_fp
suspnd
suspnd_bit
swap
swdte
swdte_bit
swdten
swdten_bit
sync
sync_bit
sync_txsta_bit
sync1
sync1_bit
sync2
sync2_bit
t08bit
t08bit_bit
t0cki0
t0cki0_bit
t0cki1
t0cki1_bit
t0cki2
t0cki2_bit
t0cki3
t0cki3_bit
t0cki4
t0cki4_bit
t0con
t0cs
t0cs_bit
t0ie
t0ie_bit
t0if
t0if_bit
t0ip
t0ip_bit
t0ps0
t0ps0_bit
t0ps1
t0ps1_bit
t0ps2
t0ps2_bit
t0se
t0se_bit
t1ck
t1ck_bit
t1ckps0
t1ckps0_bit
t1ckps01
t1ckps01_bit
t1ckps1
t1ckps1_bit
t1ckps11
t1ckps11_bit
t1con
t1done
t1done_bit
t1g0
t1g0_bit
t1g1
t1g1_bit
t1g2
t1g2_bit
t1g3
t1g3_bit
t1g4
t1g4_bit
t1gcon
t1ggo
t1ggo_bit
t1ggo_t1done
t1ggo_t1done_bit
t1gpol
t1gpol_bit
t1gspm
t1gspm_bit
t1gss0
t1gss0_bit
t1gss1
t1gss1_bit
t1gtm
t1gtm_bit
t1gval
t1gval_bit
t1oscen
t1oscen_bit
t1oscen1
t1oscen1_bit
t1osi
t1osi_bit
t1oso
t1oso_bit
t1run
t1run_bit
t1sync
t1sync_bit
t1sync1
t1sync1_bit
t2ckps0
t2ckps0_bit
t2ckps1
t2ckps1_bit
t2con
t2outps0
t2outps0_bit
t2outps1
t2outps1_bit
t2outps2
t2outps2_bit
t2outps3
t2outps3_bit
t3ccp1
t3ccp1_bit
t3ccp2
t3ccp2_bit
t3cki0
t3cki0_bit
t3cki1
t3cki1_bit
t3cki2
t3cki2_bit
t3cki3
t3cki3_bit
t3cki4
t3cki4_bit
t3ckps0
t3ckps0_bit
t3ckps1
t3ckps1_bit
t3con
t3done
t3done_bit
t3g0
t3g0_bit
t3g1
t3g1_bit
t3g2
t3g2_bit
t3g3
t3g3_bit
t3g4
t3g4_bit
t3gcon
t3ggo
t3ggo_bit
t3ggo_t3done
t3ggo_t3done_bit
t3gpol
t3gpol_bit
t3gspm
t3gspm_bit
t3gss0
t3gss0_bit
t3gss1
t3gss1_bit
t3gtm
t3gtm_bit
t3gval
t3gval_bit
t3sync
t3sync_bit
t4ckps0
t4ckps0_bit
t4ckps1
t4ckps1_bit
t4con
t4outps0
t4outps0_bit
t4outps1
t4outps1_bit
t4outps2
t4outps2_bit
t4outps3
t4outps3_bit
tablat
tblptr
tblptrh
tblptrl
tblptru
tblptru0
tblptru0_bit
tblptru1
tblptru1_bit
tblptru2
tblptru2_bit
tblptru3
tblptru3_bit
tblptru4
tblptru4_bit
tclkcon
tgen
tgen_bit
tmr0h
tmr0ie
tmr0ie_bit
tmr0if
tmr0if_bit
tmr0ip
tmr0ip_bit
tmr0l
tmr0on
tmr0on_bit
tmr1cs0
tmr1cs0_bit
tmr1cs01
tmr1cs01_bit
tmr1cs1
tmr1cs1_bit
tmr1cs11
tmr1cs11_bit
tmr1ge
tmr1ge_bit
tmr1h
tmr1ie
tmr1ie_bit
tmr1if
tmr1if_bit
tmr1ip
tmr1ip_bit
tmr1l
tmr1on
tmr1on_bit
tmr2
tmr2ie
tmr2ie_bit
tmr2if
tmr2if_bit
tmr2ip
tmr2ip_bit
tmr2on
tmr2on_bit
tmr3cs0
tmr3cs0_bit
tmr3cs1
tmr3cs1_bit
tmr3ge
tmr3ge_bit
tmr3gie
tmr3gie_bit
tmr3gif
tmr3gif_bit
tmr3gip
tmr3gip_bit
tmr3h
tmr3ie
tmr3ie_bit
tmr3if
tmr3if_bit
tmr3ip
tmr3ip_bit
tmr3l
tmr3on
tmr3on_bit
tmr4
tmr4ie
tmr4ie_bit
tmr4if
tmr4if_bit
tmr4ip
tmr4ip_bit
tmr4on
tmr4on_bit
to_
to__bit
tolower
tosh
tosl
tosu
toupper
trisa
trisa0
trisa0_bit
trisa1
trisa1_bit
trisa2
trisa2_bit
trisa3
trisa3_bit
trisa5
trisa5_bit
trisa6
trisa6_bit
trisa7
trisa7_bit
trisb
trisb0
trisb0_bit
trisb1
trisb1_bit
trisb2
trisb2_bit
trisb3
trisb3_bit
trisb4
trisb4_bit
trisb5
trisb5_bit
trisb6
trisb6_bit
trisb7
trisb7_bit
trisc
trisc0
trisc0_bit
trisc1
trisc1_bit
trisc2
trisc2_bit
trisc4
trisc4_bit
trisc5
trisc5_bit
trisc6
trisc6_bit
trisc7
trisc7_bit
trmt
trmt_bit
trmt_txsta_bit
trmt1
trmt1_bit
trmt2
trmt2_bit
trnie
trnie_bit
trnif
trnif_bit
tun0
tun0_bit
tun1
tun1_bit
tun2
tun2_bit
tun3
tun3_bit
tun4
tun4_bit
tun5
tun5_bit
tx1
tx1_bit
tx1ie
tx1ie_bit
tx1if
tx1if_bit
tx1ip
tx1ip_bit
tx2ie
tx2ie_bit
tx2if
tx2if_bit
tx2ip
tx2ip_bit
tx8_9
tx8_9_bit
tx9
tx9_bit
tx9_txsta_bit
tx91
tx91_bit
tx92
tx92_bit
tx9d
tx9d_bit
tx9d_txsta_bit
tx9d1
tx9d1_bit
tx9d2
tx9d2_bit
txaddrh
txaddrl
txckp
txckp_baudcon_bit
txckp_bit
txd8
txd8_bit
txen
txen_bit
txen_txsta_bit
txen1
txen1_bit
txen2
txen2_bit
txie
txie_bit
txif
txif_bit
txinc
txinc_bit
txip
txip_bit
txreg
txreg1
txreg2
txsta
txsta1
txsta2
u1od
u1od_bit
u2od
u2od_bit
ua
ua_bit
ua_ssp1stat_bit
ua1
ua1_bit
uaddr
uart_data_ready
uart_rd_ptr
uart_rdy_ptr
uart_read
uart_read_text
uart_remappable_data_ready
uart_remappable_init
uart_remappable_read
uart_remappable_read_text
uart_remappable_tx_idle
uart_remappable_write
uart_remappable_write_text
uart_set_active
uart_tx_idle
uart_tx_idle_ptr
uart_wr_ptr
uart_write
uart_write_text
uart1_data_ready
uart1_init
uart1_read
uart1_read_text
uart1_tx_idle
uart1_write
uart1_write_text
ucfg
ucon
ueie
ueir
uep0
uep1
uep10
uep11
uep12
uep13
uep14
uep15
uep2
uep3
uep4
uep5
uep6
uep7
uep8
uep9
uerrie
uerrie_bit
uerrif
uerrif_bit
ufrmh
ufrml
uie
uir
ulpen
ulpen_bit
ulplvl
ulplvl_bit
ulpsink
ulpsink_bit
ulpwdis
ulpwdis_bit
ulpwu
ulpwu_bit
unlock_iolock
uoemon
uoemon_bit
upuen
upuen_bit
urstie
urstie_bit
urstif
urstif_bit
usb_break
usb_config_dsc_ptr
usb_hid_ep
usb_hid_rpt_size
usb_init_desc
usb_interrupt
usb_interrupt_proc
usb_max_power
usb_polling_proc
usb_product_id
usb_self_power
usb_string_dsc_ptr
usb_transfer_type
usb_vendor_id
usben
usben_bit
usbie
usbie_bit
usbif
usbif_bit
usbip
usbip_bit
ustat
uteye
uteye_bit
utrdis
utrdis_bit
vbg2en
vbg2en_bit
vbgen
vbgen_bit
vcfg0
vcfg0_bit
vcfg1
vcfg1_bit
vdelay_advanced_ms
vdelay_ms
vdirmag
vdirmag_bit
vm
vm_bit
vmo
vmo_bit
volctrl
vp
vp_bit
vpo
vpo_bit
vref_minus
vref_minus_bit
vref_plus
vref_plus_bit
w
wcol
wcol_bit
wcol_ssp1con1_bit
wcol1
wcol1_bit
wdtcon
word2double
wordtohex
wordtostr
wordtostrwithzeros
wprog
wprog_bit
wr
wr_bit
wreg
wren
wren_bit
wrerr
wrerr_bit
writebuff
wue
wue_baudcon_bit
wue_bit
z
z_bit
