[DEVICE]
Name=P18F26J50
Clock=48000000
[MEMORY_MODEL]
Value=0
[BUILD_TYPE]
Value=0
[ACTIVE_TAB]
Value=irct.c
[USE_EEPROM]
Value=0
[USE_HEAP]
Value=0
[HEAP_SIZE]
Value=0
[EEPROM_DEFINITION]
Value=
[FILES]
Count=2
File0=irct.c
File1=USBdsc.c
[BINARIES]
Count=0
[IMAGES]
Count=0
ActiveImageIndex=-1
[OPENED_FILES]
Count=2
File0=irct.c
File1=USBdsc.c
[EEPROM]
Count=0
[ACTIVE_COMMENTS_FILES]
Count=0
[OTHER_FILES]
Count=0
[SEARCH_PATH]
Count=3
Path0=C:\Users\Public\Documents\Mikroelektronika\mikroC PRO for PIC\Defs\
Path1=C:\Users\Public\Documents\Mikroelektronika\mikroC PRO for PIC\uses\P18\
Path2=C:\Users\Lenovo\Desktop\irrecv\
[HEADER_PATH]
Count=0
[HEADERS]
Count=0
[PLDS]
Count=0
[Useses]
Count=7
File0=Conversions
File1=C_String
File2=USB
File3=UART_Remappable
File4=Peripheral_Pin_Select
File5=UART
File6=C_Type
[EXPANDED_NODES]
Node0=Sources
Count=1
