(kicad_pcb (version 4) (host pcbnew 4.0.6)

  (general
    (links 25)
    (no_connects 5)
    (area 60.174999 82.924999 210.325001 108.075001)
    (thickness 1.6)
    (drawings 8)
    (tracks 58)
    (zones 0)
    (modules 11)
    (nets 18)
  )

  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 2)
    (via_drill 1.5)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 2)
    (uvia_drill 1.5)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(J2-Pad3)")
  (net 4 "Net-(J2-Pad2)")
  (net 5 "Net-(J2-Pad5)")
  (net 6 "Net-(J3-Pad3)")
  (net 7 "Net-(J3-Pad2)")
  (net 8 "Net-(J3-Pad5)")
  (net 9 "Net-(J4-Pad3)")
  (net 10 "Net-(J4-Pad2)")
  (net 11 "Net-(J4-Pad5)")
  (net 12 "Net-(J5-Pad3)")
  (net 13 "Net-(J5-Pad2)")
  (net 14 "Net-(J5-Pad5)")
  (net 15 "Net-(J6-Pad3)")
  (net 16 "Net-(J6-Pad2)")
  (net 17 "Net-(J6-Pad5)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 2)
    (via_drill 1.5)
    (uvia_dia 2)
    (uvia_drill 1.5)
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad5)")
  )

  (net_class PWR_Rail ""
    (clearance 0.25)
    (trace_width 2.5)
    (via_dia 3)
    (via_drill 2)
    (uvia_dia 3)
    (uvia_drill 2)
    (add_net GND)
    (add_net VCC)
  )

  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 563007E4) (tstamp 5906465F)
    (at 75 93 180)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (path /59064B2E)
    (fp_text reference J1 (at 2.5 5.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Screw_Terminal_1x02 (at 2.5 -6.6 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.7 -5.4) (end 7.7 -5.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 4.8) (end -2.7 -5.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.7 4.8) (end -2.7 4.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.7 -5.4) (end 7.7 4.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.5 4.1) (end 2.5 4.6) (layer F.SilkS) (width 0.15))
    (fp_circle (center 5 0.1) (end 3 0.1) (layer F.SilkS) (width 0.15))
    (fp_circle (center 0 0.1) (end 2 0.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.5 2.6) (end 7.5 2.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.5 -2.3) (end 7.5 -2.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.5 4.1) (end 7.5 4.1) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.5 4.6) (end 7.5 4.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.5 4.6) (end 7.5 -5.2) (layer F.SilkS) (width 0.15))
    (fp_line (start 7.5 -5.2) (end -2.5 -5.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.5 -5.2) (end -2.5 4.6) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors:USB_A (layer F.Cu) (tedit 5543E289) (tstamp 59064669)
    (at 90 100)
    (descr "USB A connector")
    (tags "USB USB_A")
    (path /5905FD5D)
    (fp_text reference J2 (at 0 -2.35) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USB_A (at 3.84 7.44) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.3 13.2) (end -5.3 -1.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.95 -1.4) (end 11.95 13.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 13.2) (end 11.95 13.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -1.4) (end 11.95 -1.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.05 -1.14) (end 11.05 1.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.94 -1.14) (end -3.94 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 -1.14) (end -3.94 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 12.95) (end -3.94 12.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 4.15) (end 11.05 12.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.94 4.35) (end -3.94 12.95) (layer F.SilkS) (width 0.12))
    (pad 4 thru_hole circle (at 7.11 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 4.57 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 5 thru_hole circle (at 10.16 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad5)"))
    (pad 5 thru_hole circle (at -3.56 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad5)"))
    (model Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Connectors:USB_A (layer F.Cu) (tedit 5543E289) (tstamp 59064673)
    (at 115 100)
    (descr "USB A connector")
    (tags "USB USB_A")
    (path /5905FCF0)
    (fp_text reference J3 (at 0 -2.35) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USB_A (at 3.84 7.44) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.3 13.2) (end -5.3 -1.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.95 -1.4) (end 11.95 13.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 13.2) (end 11.95 13.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -1.4) (end 11.95 -1.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.05 -1.14) (end 11.05 1.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.94 -1.14) (end -3.94 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 -1.14) (end -3.94 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 12.95) (end -3.94 12.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 4.15) (end 11.05 12.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.94 4.35) (end -3.94 12.95) (layer F.SilkS) (width 0.12))
    (pad 4 thru_hole circle (at 7.11 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 4.57 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 5 thru_hole circle (at 10.16 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad5)"))
    (pad 5 thru_hole circle (at -3.56 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad5)"))
    (model Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Connectors:USB_A (layer F.Cu) (tedit 5543E289) (tstamp 5906467D)
    (at 140 100)
    (descr "USB A connector")
    (tags "USB USB_A")
    (path /5905FDC0)
    (fp_text reference J4 (at 0 -2.35) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USB_A (at 3.84 7.44) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.3 13.2) (end -5.3 -1.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.95 -1.4) (end 11.95 13.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 13.2) (end 11.95 13.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -1.4) (end 11.95 -1.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.05 -1.14) (end 11.05 1.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.94 -1.14) (end -3.94 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 -1.14) (end -3.94 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 12.95) (end -3.94 12.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 4.15) (end 11.05 12.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.94 4.35) (end -3.94 12.95) (layer F.SilkS) (width 0.12))
    (pad 4 thru_hole circle (at 7.11 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 4.57 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 5 thru_hole circle (at 10.16 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad5)"))
    (pad 5 thru_hole circle (at -3.56 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad5)"))
    (model Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Connectors:USB_A (layer F.Cu) (tedit 5543E289) (tstamp 59064687)
    (at 165 100)
    (descr "USB A connector")
    (tags "USB USB_A")
    (path /5905F932)
    (fp_text reference J5 (at 0 -2.35) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USB_A (at 3.84 7.44) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.3 13.2) (end -5.3 -1.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.95 -1.4) (end 11.95 13.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 13.2) (end 11.95 13.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -1.4) (end 11.95 -1.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.05 -1.14) (end 11.05 1.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.94 -1.14) (end -3.94 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 -1.14) (end -3.94 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 12.95) (end -3.94 12.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 4.15) (end 11.05 12.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.94 4.35) (end -3.94 12.95) (layer F.SilkS) (width 0.12))
    (pad 4 thru_hole circle (at 7.11 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 4.57 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J5-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 5 thru_hole circle (at 10.16 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 14 "Net-(J5-Pad5)"))
    (pad 5 thru_hole circle (at -3.56 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 14 "Net-(J5-Pad5)"))
    (model Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Connectors:USB_A (layer F.Cu) (tedit 5543E289) (tstamp 59064691)
    (at 190 100)
    (descr "USB A connector")
    (tags "USB USB_A")
    (path /5905FB99)
    (fp_text reference J6 (at 0 -2.35) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USB_A (at 3.84 7.44) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.3 13.2) (end -5.3 -1.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.95 -1.4) (end 11.95 13.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 13.2) (end 11.95 13.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 -1.4) (end 11.95 -1.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.05 -1.14) (end 11.05 1.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.94 -1.14) (end -3.94 0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 -1.14) (end -3.94 -1.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 12.95) (end -3.94 12.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 11.05 4.15) (end 11.05 12.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.94 4.35) (end -3.94 12.95) (layer F.SilkS) (width 0.12))
    (pad 4 thru_hole circle (at 7.11 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 4.57 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J6-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 5 thru_hole circle (at 10.16 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 17 "Net-(J6-Pad5)"))
    (pad 5 thru_hole circle (at -3.56 2.67 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 17 "Net-(J6-Pad5)"))
    (model Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 59064697)
    (at 198.5 93 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59063FB6)
    (fp_text reference R1 (at 5.08 -2.31 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100 (at 5.08 2.31 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.87 -1.31) (end 1.87 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 1.31) (end 8.29 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.29 1.31) (end 8.29 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.29 -1.31) (end 1.87 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.98 0) (end 1.87 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.18 0) (end 8.29 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 11.25 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.25 1.6) (end 11.25 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.25 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J6-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J6-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 5906469D)
    (at 123.5 93 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /5906401F)
    (fp_text reference R2 (at 5.08 -2.31 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100 (at 5.08 2.31 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.87 -1.31) (end 1.87 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 1.31) (end 8.29 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.29 1.31) (end 8.29 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.29 -1.31) (end 1.87 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.98 0) (end 1.87 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.18 0) (end 8.29 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 11.25 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.25 1.6) (end 11.25 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.25 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 590646A3)
    (at 98.5 93 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /590640AE)
    (fp_text reference R3 (at 5.08 -2.31 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100 (at 5.08 2.31 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.87 -1.31) (end 1.87 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 1.31) (end 8.29 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.29 1.31) (end 8.29 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.29 -1.31) (end 1.87 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.98 0) (end 1.87 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.18 0) (end 8.29 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 11.25 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.25 1.6) (end 11.25 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.25 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 590646A9)
    (at 148.5 93 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59064154)
    (fp_text reference R4 (at 5.08 -2.31 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100 (at 5.08 2.31 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.87 -1.31) (end 1.87 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 1.31) (end 8.29 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.29 1.31) (end 8.29 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.29 -1.31) (end 1.87 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.98 0) (end 1.87 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.18 0) (end 8.29 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 11.25 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.25 1.6) (end 11.25 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.25 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706) (tstamp 590646AF)
    (at 173.5 93 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /59063F2F)
    (fp_text reference R5 (at 5.08 -2.31 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100 (at 5.08 2.31 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.87 -1.31) (end 1.87 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 1.31) (end 8.29 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.29 1.31) (end 8.29 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.29 -1.31) (end 1.87 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.98 0) (end 1.87 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.18 0) (end 8.29 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 11.25 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.25 1.6) (end 11.25 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.25 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J5-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J5-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_circle (center 207.25 105) (end 209.25 105) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 207.25 86) (end 209.25 86) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 63.25 86) (end 61.25 86) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 63.25 105) (end 61.25 105) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 210.25 108) (end 60.25 108) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 210.25 83) (end 210.25 108) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 60.25 83) (end 210.25 83) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 60.25 108) (end 60.25 83) (angle 90) (layer Edge.Cuts) (width 0.15))

  (segment (start 90 100) (end 83 93) (width 2.5) (layer B.Cu) (net 1) (status 400000))
  (segment (start 83 93) (end 75 93) (width 2.5) (layer B.Cu) (net 1) (tstamp 59065C85) (status 800000))
  (segment (start 115 100) (end 107 92) (width 2.5) (layer B.Cu) (net 1) (status 400000))
  (segment (start 107 92) (end 107 85.25) (width 2.5) (layer B.Cu) (net 1) (tstamp 59065C6A))
  (segment (start 140 100) (end 131.25 91.25) (width 2.5) (layer B.Cu) (net 1) (status 400000))
  (segment (start 131.25 91.25) (end 131.25 85.25) (width 2.5) (layer B.Cu) (net 1) (tstamp 59065C3A))
  (segment (start 165 100) (end 156.25 91.25) (width 2.5) (layer B.Cu) (net 1) (status 400000))
  (segment (start 156.25 91.25) (end 156.25 85.25) (width 2.5) (layer B.Cu) (net 1) (tstamp 59065C13))
  (segment (start 75 93) (end 75 85.25) (width 2.5) (layer B.Cu) (net 1) (status 400000))
  (segment (start 179.75 89.75) (end 190 100) (width 2.5) (layer B.Cu) (net 1) (tstamp 59065BF6) (status 800000))
  (segment (start 179.75 85.5) (end 179.75 89.75) (width 2.5) (layer B.Cu) (net 1) (tstamp 59065BE1))
  (segment (start 179.5 85.25) (end 179.75 85.5) (width 2.5) (layer B.Cu) (net 1) (tstamp 59065B9E))
  (segment (start 75 85.25) (end 107 85.25) (width 2.5) (layer B.Cu) (net 1) (tstamp 59065B99))
  (segment (start 107 85.25) (end 131.25 85.25) (width 2.5) (layer B.Cu) (net 1) (tstamp 59065C7C))
  (segment (start 131.25 85.25) (end 156.25 85.25) (width 2.5) (layer B.Cu) (net 1) (tstamp 59065C54))
  (segment (start 156.25 85.25) (end 179.5 85.25) (width 2.5) (layer B.Cu) (net 1) (tstamp 59065C22))
  (segment (start 122.11 100) (end 122.11 106) (width 2.5) (layer B.Cu) (net 2) (status 400000))
  (segment (start 122.11 106) (end 122 106) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E75))
  (segment (start 97.11 100) (end 97.11 106) (width 2.5) (layer B.Cu) (net 2) (status 400000))
  (segment (start 97.11 106) (end 97.25 106) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E70))
  (segment (start 147.11 100) (end 147.11 106) (width 2.5) (layer B.Cu) (net 2) (status 400000))
  (segment (start 147.11 106) (end 147 106) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E5A))
  (segment (start 172.11 100) (end 172.11 106) (width 2.5) (layer B.Cu) (net 2) (status 400000))
  (segment (start 172 105.75) (end 172 106) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E52))
  (segment (start 172 105.89) (end 172 105.75) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E51))
  (segment (start 172.11 106) (end 172 105.89) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E4D))
  (segment (start 70 93) (end 70 101.75) (width 2.5) (layer B.Cu) (net 2) (status 400000))
  (segment (start 197.11 102.14) (end 197.11 100) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E23) (status 800000))
  (segment (start 193.25 106) (end 197.11 102.14) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E01))
  (segment (start 74.25 106) (end 97.25 106) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065DE9))
  (segment (start 97.25 106) (end 122 106) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E73))
  (segment (start 122 106) (end 143.75 106) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E78))
  (segment (start 143.75 106) (end 147 106) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E38))
  (segment (start 147 106) (end 167.25 106) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E6E))
  (segment (start 167.25 106) (end 169.25 106) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E31))
  (segment (start 169.25 106) (end 172 106) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E43))
  (segment (start 172 106) (end 193.25 106) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065E53))
  (segment (start 70 101.75) (end 74.25 106) (width 2.5) (layer B.Cu) (net 2) (tstamp 59065DE4))
  (segment (start 94.57 100) (end 94.57 96.93) (width 0.6) (layer B.Cu) (net 3) (status 400000))
  (segment (start 94.57 96.93) (end 98.5 93) (width 0.6) (layer B.Cu) (net 3) (tstamp 59065CBE) (status 800000))
  (segment (start 92.54 100) (end 92.54 97.2) (width 0.6) (layer B.Cu) (net 4) (status 400000))
  (segment (start 92.54 97.2) (end 88.34 93) (width 0.6) (layer B.Cu) (net 4) (tstamp 59065CB8) (status 800000))
  (segment (start 119.57 100) (end 119.57 96.93) (width 0.6) (layer B.Cu) (net 6) (status 400000))
  (segment (start 119.57 96.93) (end 123.5 93) (width 0.6) (layer B.Cu) (net 6) (tstamp 59065D98) (status 800000))
  (segment (start 117.54 100) (end 117.54 97.2) (width 0.6) (layer B.Cu) (net 7) (status 400000))
  (segment (start 117.54 97.2) (end 113.34 93) (width 0.6) (layer B.Cu) (net 7) (tstamp 59065CC7) (status 800000))
  (segment (start 144.57 100) (end 144.57 96.93) (width 0.6) (layer B.Cu) (net 9) (status 400000))
  (segment (start 144.57 96.93) (end 148.5 93) (width 0.6) (layer B.Cu) (net 9) (tstamp 59065DA1) (status 800000))
  (segment (start 142.54 100) (end 142.54 97.2) (width 0.6) (layer B.Cu) (net 10) (status 400000))
  (segment (start 142.54 97.2) (end 138.34 93) (width 0.6) (layer B.Cu) (net 10) (tstamp 59065D9D) (status 800000))
  (segment (start 169.57 100) (end 169.57 96.93) (width 0.6) (layer B.Cu) (net 12) (status 400000))
  (segment (start 169.57 96.93) (end 173.5 93) (width 0.6) (layer B.Cu) (net 12) (tstamp 59065DB1) (status 800000))
  (segment (start 167.54 100) (end 167.54 97.2) (width 0.6) (layer B.Cu) (net 13) (status 400000))
  (segment (start 167.54 97.2) (end 163.34 93) (width 0.6) (layer B.Cu) (net 13) (tstamp 59065DAD) (status 800000))
  (segment (start 194.57 100) (end 194.57 96.93) (width 0.6) (layer B.Cu) (net 15) (status 400000))
  (segment (start 194.57 96.93) (end 198.5 93) (width 0.6) (layer B.Cu) (net 15) (tstamp 59065DA9) (status 800000))
  (segment (start 192.54 100) (end 192.54 97.2) (width 0.6) (layer B.Cu) (net 16) (status 400000))
  (segment (start 192.54 97.2) (end 188.34 93) (width 0.6) (layer B.Cu) (net 16) (tstamp 59065DA5) (status 800000))

)
