/** \file
 *
 *  This file contains special DoxyGen information for the generation of the main page and other special
 *  documentation pages. It is not a project source file.
 */

/** \page Page_VIDPID VID and PID values
 *
 *  \section Sec_VIDPID_Allocations
 *  The LUFA library uses VID/PID combinations generously donated by Atmel. The following VID/PID combinations
 *  are used within the LUFA demos, and thus may be re-used by derivations of each demo. Free PID values may be
 *  used by future LUFA demo projects.
 *
 *  <b>These VID/PID values should not be used in commercial designs under any circumstances.</b> Private projects
 *  may use the following values freely, but must accept any collisions due to other LUFA derived private projects
 *  sharing identical values. It is suggested that private projects using interfaces compatible with existing
 *  demos share the same VID/PID value.
 *
 *  <table>
 *
 *   <tr>
 *    <td>
 *     <b>VID</b>
 *    </td>
 *    <td>
 *     <b>PID</b>
 *    </td>
 *    <td>
 *     <b>Usage</b>
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2040
 *    </td>
 *    <td>
 *     Test VID/PID (See below)
 *    </td>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2041
 *    </td>
 *    <td>
 *     Mouse Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2042
 *    </td>
 *    <td>
 *     Keyboard Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2043
 *    </td>
 *    <td>
 *     Joystick Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2044
 *    </td>
 *    <td>
 *     CDC Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2045
 *    </td>
 *    <td>
 *     Mass Storage Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2046
 *    </td>
 *    <td>
 *     Audio Output Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2047
 *    </td>
 *    <td>
 *     Audio Input Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2048
 *    </td>
 *    <td>
 *     MIDI Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2049
 *    </td>
 *    <td>
 *     MagStripe Project
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x204A
 *    </td>
 *    <td>
 *     CDC Bootloader
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x204B
 *    </td>
 *    <td>
 *     USB to Serial Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x204C
 *    </td>
 *    <td>
 *     RNDIS Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x204D
 *    </td>
 *    <td>
 *     Combined Keyboard and Mouse Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x204E
 *    </td>
 *    <td>
 *     Dual CDC Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x204F
 *    </td>
 *    <td>
 *     Generic HID Demo Application
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2060
 *    </td>
 *    <td>
 *     Benito Programmer Project
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2061
 *    </td>
 *    <td>
 *     Combined Mass Storage and Keyboard Demo
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2062
 *    </td>
 *    <td>
 *     Combined CDC and Mouse Demo
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2063
 *    </td>
 *    <td>
 *     Mass Storage/HID Interface Datalogger Project
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2064
 *    </td>
 *    <td>
 *     Interfaceless Control-Only LUFA Devices
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2065
 *    </td>
 *    <td>
 *     Test and Measurement Demo
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2066
 *    </td>
 *    <td>
 *     Multiple Report Keyboard/Mouse HID Demo
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2067
 *    </td>
 *    <td>
 *     HID Class Bootloader
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2068
 *    </td>
 *    <td>
 *     Virtual Serial/Mass Storage Demo
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x2069
 *    </td>
 *    <td>
 *     Webserver Project
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x206A
 *    </td>
 *    <td>
 *     Media Control Project
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x206B
 *    </td>
 *    <td>
 *     <i>Currently Unallocated</i>
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x206C
 *    </td>
 *    <td>
 *     <i>Currently Unallocated</i>
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x206D
 *    </td>
 *    <td>
 *     <i>Currently Unallocated</i>
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x206E
 *    </td>
 *    <td>
 *     <i>Currently Unallocated</i>
 *    </td>
 *   </tr>
 *
 *   <tr>
 *    <td>
 *     0x03EB
 *    </td>
 *    <td>
 *     0x206F
 *    </td>
 *    <td>
 *     <i>Currently Unallocated</i>
 *    </td>
 *   </tr>
 *
 *  </table>
 *
 *  \section Sec_Test_VIDPID The Test VID/PID Combination:
 *  For use in testing of LUFA powered devices during development only, by non-commercial entities.
 *  All devices must accept collisions on this VID/PID range (from other in-development LUFA devices)
 *  to be resolved by using a unique release number in the Device Descriptor. No devices using this
 *  VID/PID combination may be released to the general public.
 */

