<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="-0.25" y1="1" x2="0.75" y2="0" width="0" layer="20" curve="90"/>
<wire x1="0.75" y1="0" x2="1.25" y2="0" width="0" layer="20"/>
<wire x1="1.25" y1="0" x2="12.75" y2="0" width="0" layer="20"/>
<wire x1="12.75" y1="0" x2="13.75" y2="1" width="0" layer="20" curve="90"/>
<wire x1="13.75" y1="1" x2="13.75" y2="9" width="0" layer="20"/>
<wire x1="13.75" y1="9" x2="12.75" y2="10" width="0" layer="20" curve="90"/>
<wire x1="12.75" y1="10" x2="1.25" y2="10" width="0" layer="20"/>
<wire x1="1.25" y1="10" x2="0.75" y2="10" width="0" layer="20"/>
<wire x1="0.75" y1="10" x2="-0.25" y2="9" width="0" layer="20" curve="90"/>
<wire x1="-0.25" y1="9" x2="-0.25" y2="1" width="0" layer="20"/>
</plain>
<libraries>
<library name="we-chip">
<description>Chips, ICs...</description>
<packages>
<package name="QFN20-PAD">
</package>
</packages>
</library>
<library name="we-rcl">
<description>R, C, L, Diodes, Crystals</description>
<packages>
<package name="C0402">
</package>
<package name="SOD882">
</package>
<package name="PAD-1.0">
<description>Pad with cream</description>
</package>
</packages>
</library>
<library name="we-symbol">
<description>Symbols, Logos...</description>
<packages>
<package name="PASSER_07MM">
</package>
</packages>
</library>
<library name="we-con">
<description>Connectors, Sockets...</description>
<packages>
<package name="USB-MICROB-10118194">
<description>USB Micro-B Surface Mounted
&lt;br&gt;
FCI 10118194-0001LF</description>
</package>
</packages>
</library>
<library name="we-switch">
<description>Switches</description>
<packages>
<package name="PTS840P">
<description>C&amp;K Components PTS840 PM SMTR LFS or PTS840 PK SMTR LFS</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="thar">
<packages>
<package name="FM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="we-symbol" package="PASSER_07MM" value="PASSER-07"/>
<element name="X2" library="we-symbol" package="PASSER_07MM" value="PASSER-07"/>
<element name="X3" library="we-symbol" package="PASSER_07MM" value="PASSER-07"/>
<element name="C1" library="we-rcl" package="C0402" value="100n">
<attribute name="NAME"/>
</element>
<element name="IC2" library="we-chip" package="QFN20-PAD" value="ATTINY85-MU">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="ATTINY85-20MURDKR-ND"/>
</element>
<element name="J1" library="we-con" package="USB-MICROB-10118194" value="USB-MICROB-2">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="609-4618-6-ND "/>
</element>
<element name="R3" library="we-rcl" package="C0402" value="100">
<attribute name="NAME"/>
</element>
<element name="R2" library="we-rcl" package="C0402" value="100">
<attribute name="NAME"/>
</element>
<element name="R4" library="we-rcl" package="C0402" value="1k5">
<attribute name="NAME"/>
</element>
<element name="R1" library="we-rcl" package="C0402" value="3k9">
<attribute name="NAME"/>
</element>
<element name="D2" library="we-rcl" package="SOD882" value="Z3V6">
<attribute name="NAME"/>
</element>
<element name="D1" library="we-rcl" package="SOD882" value="Z3V6">
<attribute name="NAME"/>
</element>
<element name="SW1" library="we-switch" package="PTS840P" value="SW-TACTILE-PTS840P">
<attribute name="DIGIKEY" value="CKN10511DKR-ND"/>
<attribute name="NAME"/>
</element>
<element name="MISO" library="we-rcl" package="PAD-1.0" value="PAD-1.0">
<attribute name="NAME"/>
</element>
<element name="SCK" library="we-rcl" package="PAD-1.0" value="PAD-1.0">
<attribute name="NAME"/>
</element>
<element name="RST" library="we-rcl" package="PAD-1.0" value="PAD-1.0">
<attribute name="NAME"/>
</element>
<element name="JP1" library="pinhead" package="1X03" value=""/>
<element name="U$1" library="thar" package="FM" value="CARRIER_NCFM"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="J1" pad="GND"/>
<contactref element="D2" pad="A"/>
<contactref element="D1" pad="A"/>
<contactref element="J1" pad="SHLD1"/>
<contactref element="J1" pad="SHLD2"/>
<contactref element="IC2" pad="TP"/>
<contactref element="J1" pad="SHLD3"/>
<contactref element="J1" pad="SHLD4"/>
<contactref element="J1" pad="SHLD5"/>
<contactref element="J1" pad="SHLD6"/>
<contactref element="J1" pad="SHLD7"/>
<contactref element="J1" pad="SHLD8"/>
<contactref element="SW1" pad="4"/>
<contactref element="SW1" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="C1" pad="2"/>
<contactref element="IC2" pad="15"/>
<contactref element="R1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="J1" pad="VBUS"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="PB3">
<contactref element="IC2" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="PB4">
<contactref element="IC2" pad="5"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="D_P">
<contactref element="R3" pad="2"/>
<contactref element="J1" pad="D+"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="PB5">
<contactref element="IC2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="RST" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC2" pad="11"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="J1" pad="D-"/>
<contactref element="D2" pad="C"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC2" pad="14"/>
<contactref element="SCK" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC2" pad="12"/>
<contactref element="MISO" pad="1"/>
<contactref element="SW1" pad="2"/>
<contactref element="SW1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
