<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="1.905" y1="-3.81" x2="87.61" y2="-3.81" width="0" layer="20"/>
<wire x1="87.61" y1="-3.81" x2="87.61" y2="66.98" width="0" layer="20"/>
<wire x1="87.61" y1="66.98" x2="1.905" y2="66.98" width="0" layer="20"/>
<wire x1="1.905" y1="66.98" x2="1.905" y2="-3.81" width="0" layer="20"/>
<text>5V</text>
<text>12V</text>
<text>FPGA</text>
<text>Globe</text>
<text>Capteur</text>
<text>12V</text>
<text>5V</text>
<text>Moteur</text>
<text>FPGA</text>
<text>J_FPGA</text>
<text>J_Régu</text>
<text>FPGA_5V</text>
<text>FPGA_12V</text>
</plain>
<libraries>
<library name="transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220BV">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="fuse">
<description>&lt;b&gt;Fuses and Fuse Holders&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LITTLEFUSE">
<description>&lt;B&gt;LITTLEFUSE&lt;/B&gt;&lt;p&gt;
Picofuse/slow Littelfuse</description>
</package>
</packages>
</library>
<library name="perso">
<packages>
<package name="PTR08100W">
</package>
<package name="TXB0104">
</package>
<package name="JUMPER_CONNECTOR">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="E2,5-7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 7 mm</description>
</package>
<package name="E7,5-16">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.62 mm, diameter 16 mm</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-jack">
<description>&lt;b&gt;Jacks&lt;/b&gt;&lt;p&gt;
Power Connectors&lt;br&gt;
Phone Connectors&lt;br&gt;
Cinch Connectors&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SPC4078">
<description>&lt;b&gt;DC POWER JACK 2.5mm&lt;/b&gt; Right Angle, Through Hole, Rated 5A at 16VDC, PC Terminals&lt;p&gt;
Source: www.spctechnology.com .. 84N1162.pdf&lt;br&gt;
Distributor: &lt;b&gt;Farnell (www.Farnell.de)&lt;/b&gt;&lt;br&gt;
Created by Robert Siegler</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA06-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA03-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-ptr500">
<description>&lt;b&gt;PTR Connectors&lt;/b&gt;&lt;p&gt;
Aug. 2004 / PTR Meßtechnik:&lt;br&gt;
Die Bezeichnung der Serie AK505 wurde geändert.&lt;br&gt;
Es handelt sich hierbei um AK500 in horizontaler Ausführung.&lt;p&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;Alte Bezeichnung&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;Neue Bezeichnung&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;AK505/2,grau&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#0000FF"&gt;AK500/2-5.0-H-GRAU&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;AK505/2DS,grau&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#0000FF"&gt;AK500/2DS-5.0-H-GRAU&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;AKZ505/2,grau&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=LEFT&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#0000FF"&gt;AKZ500/2-5.08-H-GRAU&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
  &lt;/TABLE&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="AK500/2">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="perso" package="PTR08100W" value="PTR08100W"/>
<element name="R2" library="rcl" package="0207/10" value=""/>
<element name="C8" library="rcl" package="E2,5-7" value="100 uF"/>
<element name="U$1" library="perso" package="TXB0104" value="TXB0104"/>
<element name="U$2" library="perso" package="TXB0104" value="TXB0104"/>
<element name="D1" library="diode" package="DO41-10" value="1N4004"/>
<element name="R1" library="rcl" package="0207/10" value=""/>
<element name="R3" library="rcl" package="0207/10" value=""/>
<element name="R4" library="rcl" package="0207/10" value=""/>
<element name="J1" library="con-jack" package="SPC4078" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="C1" library="rcl" package="E7,5-16" value="2.2mF"/>
<element name="R6" library="rcl" package="0207/10" value=""/>
<element name="R7" library="rcl" package="0207/10" value=""/>
<element name="R8" library="rcl" package="0207/10" value=""/>
<element name="R9" library="rcl" package="0207/10" value=""/>
<element name="R10" library="rcl" package="0207/10" value=""/>
<element name="R11" library="rcl" package="0207/10" value=""/>
<element name="SV1" library="con-lstb" package="MA06-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="SV2" library="con-lstb" package="MA06-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="SV3" library="con-lstb" package="MA03-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="X1" library="con-ptr500" package="AK500/2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="X2" library="con-ptr500" package="AK500/2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="X5" library="con-ptr500" package="AK500/2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="LED2" library="led" package="LED5MM" value=""/>
<element name="LED3" library="led" package="LED5MM" value=""/>
<element name="R12" library="rcl" package="0207/10" value=""/>
<element name="R13" library="rcl" package="0207/10" value=""/>
<element name="J2" library="con-jack" package="SPC4078" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="X6" library="con-ptr500" package="AK500/2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="OK1" library="optocoupler" package="DIL06" value="4N25M">
<attribute name="OC_NEWARK" value="98K9084"/>
<attribute name="MPN" value="4N25-M"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1021349"/>
</element>
<element name="C2" library="rcl" package="E7,5-16" value="2.2mF"/>
<element name="Q2" library="transistor-power" package="TO220BV" value="IRF9530"/>
<element name="F3" library="fuse" package="LITTLEFUSE" value="FUSELITTLEFUSE">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="F1" library="fuse" package="LITTLEFUSE" value="FUSELITTLEFUSE">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="U$4" library="perso" package="JUMPER_CONNECTOR" value="JUMPER_CONNECTOR"/>
<element name="U$5" library="perso" package="JUMPER_CONNECTOR" value="JUMPER_CONNECTOR"/>
<element name="U$6" library="perso" package="JUMPER_CONNECTOR" value="JUMPER_CONNECTOR"/>
<element name="U$7" library="perso" package="JUMPER_CONNECTOR" value="JUMPER_CONNECTOR"/>
<element name="U$10" library="perso" package="JUMPER_CONNECTOR" value="JUMPER_CONNECTOR"/>
<element name="U$12" library="perso" package="JUMPER_CONNECTOR" value="JUMPER_CONNECTOR"/>
<element name="U$3" library="perso" package="JUMPER_CONNECTOR" value="JUMPER_CONNECTOR"/>
</elements>
<signals>
<signal name="3.3V">
<contactref element="U$1" pad="VCCA"/>
<contactref element="U$2" pad="VCCA"/>
<contactref element="SV1" pad="12"/>
<contactref element="SV1" pad="11"/>
<contactref element="SV3" pad="3"/>
</signal>
<signal name="FPGA_S1">
<contactref element="U$1" pad="A1"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="FPGA_S2">
<contactref element="U$1" pad="A2"/>
<contactref element="SV1" pad="4"/>
</signal>
<signal name="FPGA_S3">
<contactref element="U$1" pad="A3"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="FPGA_S4">
<contactref element="U$1" pad="A4"/>
<contactref element="SV1" pad="8"/>
</signal>
<signal name="FPGA_S5">
<contactref element="U$2" pad="A3"/>
<contactref element="SV1" pad="1"/>
</signal>
<signal name="FPGA_S6">
<contactref element="U$2" pad="A2"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="STRIP1">
<contactref element="R6" pad="2"/>
<contactref element="SV2" pad="4"/>
</signal>
<signal name="STRIP2">
<contactref element="R7" pad="2"/>
<contactref element="SV2" pad="6"/>
</signal>
<signal name="STRIP3">
<contactref element="R8" pad="2"/>
<contactref element="SV2" pad="3"/>
</signal>
<signal name="STRIP4">
<contactref element="R9" pad="2"/>
<contactref element="SV2" pad="5"/>
</signal>
<signal name="STRIP5">
<contactref element="R10" pad="2"/>
<contactref element="SV2" pad="1"/>
</signal>
<signal name="STRIP6">
<contactref element="R11" pad="2"/>
<contactref element="SV2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C8" pad="-"/>
<contactref element="U$2" pad="GND1"/>
<contactref element="U$2" pad="GND2"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="U$1" pad="GND2"/>
<contactref element="R4" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="SV1" pad="10"/>
<contactref element="SV1" pad="9"/>
<contactref element="SV2" pad="12"/>
<contactref element="SV2" pad="10"/>
<contactref element="SV2" pad="8"/>
<contactref element="SV3" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="X1" pad="2"/>
<contactref element="X5" pad="2"/>
<contactref element="LED3" pad="K"/>
<contactref element="LED2" pad="K"/>
<contactref element="J2" pad="1"/>
<contactref element="X6" pad="2"/>
<contactref element="OK1" pad="4"/>
<contactref element="OK1" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="D1" pad="A"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="VCCB"/>
<contactref element="U$2" pad="VCCB"/>
<contactref element="SV2" pad="11"/>
<contactref element="SV2" pad="9"/>
<contactref element="SV2" pad="7"/>
<contactref element="R13" pad="1"/>
<contactref element="C2" pad="+"/>
<contactref element="F1" pad="2"/>
<contactref element="U$10" pad="P$1"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="12V_FUSIBLE">
<contactref element="C1" pad="+"/>
<contactref element="R12" pad="1"/>
<contactref element="F3" pad="2"/>
<contactref element="Q2" pad="S"/>
<contactref element="R3" pad="1"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="VO_ADJ">
<contactref element="U2" pad="5"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="FPGA_R">
<contactref element="SV1" pad="5"/>
<contactref element="SV3" pad="1"/>
</signal>
<signal name="12V">
<contactref element="J1" pad="3"/>
<contactref element="X1" pad="1"/>
<contactref element="F3" pad="1"/>
</signal>
<signal name="RES_OCTO">
<contactref element="R1" pad="1"/>
<contactref element="OK1" pad="1"/>
</signal>
<signal name="FPGA_PWM">
<contactref element="R1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="SV1" pad="7"/>
</signal>
<signal name="R_STRIP_1">
<contactref element="U$1" pad="B1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="R_STRIP_2">
<contactref element="R7" pad="1"/>
<contactref element="U$1" pad="B2"/>
</signal>
<signal name="R_STRIP_3">
<contactref element="U$1" pad="B3"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="R_STRIP_4">
<contactref element="U$1" pad="B4"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="R_STRIP_6">
<contactref element="U$2" pad="B2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="PWM_OCTO">
<contactref element="R3" pad="2"/>
<contactref element="OK1" pad="5"/>
<contactref element="Q2" pad="G"/>
</signal>
<signal name="5V_REG">
<contactref element="U2" pad="4"/>
<contactref element="C8" pad="+"/>
<contactref element="U$12" pad="P$1"/>
</signal>
<signal name="12V_REG">
<contactref element="U2" pad="2"/>
<contactref element="U$7" pad="P$1"/>
</signal>
<signal name="ALIM_FPGA">
<contactref element="X5" pad="1"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="M+">
<contactref element="D1" pad="C"/>
<contactref element="X2" pad="2"/>
<contactref element="Q2" pad="D"/>
</signal>
<signal name="RES_LED_12V">
<contactref element="R12" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="RES_LED_5V">
<contactref element="R13" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="5V_IN">
<contactref element="J2" pad="3"/>
<contactref element="X6" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="R_STRIP_5">
<contactref element="U$2" pad="B3"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$20">
</signal>
<signal name="N$21">
</signal>
<signal name="N$22">
</signal>
<signal name="N$40">
</signal>
<signal name="N$53">
</signal>
<signal name="N$57">
</signal>
<signal name="N$61">
</signal>
<signal name="N$62">
</signal>
<signal name="N$66">
</signal>
<signal name="N$101">
</signal>
</signals>
</board>
</drawing>
</eagle>
