<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="70" width="0" layer="20"/>
<wire x1="100" y1="70" x2="-0.1" y2="70" width="0" layer="20"/>
<wire x1="-0.1" y1="70" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="Q">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X04-3.5MM">
</package>
</packages>
</library>
<library name="transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220AV">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="mylibraryab">
<packages>
<package name="16PINDIL">
</package>
<package name="0411/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 15 mm</description>
</package>
<package name="LEDPACK">
</package>
<package name="PIN2">
</package>
<package name="BIGCOND">
</package>
<package name="SMALLCOND">
</package>
</packages>
</library>
<library name="Arduino-AVR-ab">
<description>&lt;b&gt;Arduino Microcontrollers&lt;/b&gt;
&lt;p&gt;
Atmel ATmega8, ATmega168: 8-bit AVR microcontrollers
&lt;p&gt;&lt;ul&gt;
&lt;li&gt;&lt;i&gt;ATmega8 was used on the original Arduino Serial and USB boards&lt;br&gt;
- 28-pin PDIP (32-lead packages also included)&lt;/i&gt;
&lt;li&gt;ATmega168 for current Arduino Diecimila and NG boards&lt;br&gt;
 - 28-pin PDIP
&lt;li&gt;ATMEGA168 for the Arduino Nano, Mini, LilyPad, Pro and so forth&lt;br&gt;
- 32-lead TQFP and 32-pad QFN/MLF
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;from Rob Faludi: www.faludi.com/projects&lt;/p&gt;</description>
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="special" package="Q" value="16Mhz"/>
<element name="C1" library="mylibraryab" package="SMALLCOND" value="22pF"/>
<element name="C2" library="mylibraryab" package="SMALLCOND" value="22pF"/>
<element name="R1" library="mylibraryab" package="0411/15" value="220"/>
<element name="LED1" library="mylibraryab" package="LEDPACK" value="LED"/>
<element name="C3" library="mylibraryab" package="BIGCOND" value="10uF"/>
<element name="R3" library="mylibraryab" package="0411/15" value="470"/>
<element name="R4" library="mylibraryab" package="0411/15" value="10k"/>
<element name="Q2" library="transistor-power" package="TO220AV" value="TIP41C"/>
<element name="LED2" library="mylibraryab" package="LEDPACK" value="LED"/>
<element name="R5" library="mylibraryab" package="0411/15" value="470"/>
<element name="LED3" library="mylibraryab" package="LEDPACK" value="LED"/>
<element name="DRUKKNOPPEN" library="adafruit" package="1X04-3.5MM" value="1X4-3.5MM"/>
<element name="R7" library="mylibraryab" package="0411/15" value="10k"/>
<element name="U$1" library="mylibraryab" package="16PINDIL" value="OPTO8OPT_16PINDIL"/>
<element name="3V" library="mylibraryab" package="PIN2" value="PIN2"/>
<element name="9V" library="mylibraryab" package="PIN2" value="PIN2"/>
<element name="MOTOR" library="mylibraryab" package="PIN2" value="PIN2"/>
<element name="U$2" library="mylibraryab" package="0411/15" value="R-BIG">
<attribute name="R" value="10K"/>
</element>
<element name="U$3" library="mylibraryab" package="0411/15" value="R-BIG">
<attribute name="R" value="10K"/>
</element>
<element name="IC1" library="Arduino-AVR-ab" package="DIL28-3" value="ATMEGA168-PU"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="LED1" pad="K"/>
<contactref element="C3" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="3V" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="VCC">
<contactref element="C3" pad="1"/>
<contactref element="DRUKKNOPPEN" pad="3"/>
<contactref element="DRUKKNOPPEN" pad="1"/>
<contactref element="3V" pad="2"/>
<contactref element="U$2" pad="1"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="20"/>
</signal>
<signal name="N$1">
<contactref element="C1" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="C2" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="+9V">
<contactref element="R5" pad="2"/>
<contactref element="LED3" pad="K"/>
<contactref element="U$1" pad="P$14"/>
<contactref element="9V" pad="2"/>
<contactref element="MOTOR" pad="2"/>
</signal>
<signal name="GND2">
<contactref element="Q2" pad="E"/>
<contactref element="R4" pad="1"/>
<contactref element="9V" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R4" pad="2"/>
<contactref element="Q2" pad="B"/>
<contactref element="U$1" pad="P$13"/>
</signal>
<signal name="N$10">
<contactref element="Q2" pad="C"/>
<contactref element="LED2" pad="K"/>
<contactref element="LED3" pad="A"/>
<contactref element="MOTOR" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R5" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="R7" pad="1"/>
<contactref element="DRUKKNOPPEN" pad="4"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="N$12">
<contactref element="DRUKKNOPPEN" pad="2"/>
<contactref element="U$3" pad="1"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="P$5"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="6"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="2"/>
<contactref element="IC1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
