<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="100" width="0" layer="20"/>
<wire x1="160" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="battery">
<description>&lt;b&gt;Lithium Batteries and NC Accus&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CH291-1220LF">
<description>&lt;b&gt;Battery Holder, SMT, 12mm&lt;/b&gt;&lt;p&gt;
multicomp PART NO. CH291-1220LF&lt;br&gt;
Source: &lt;a href="http://www.farnell.com/datasheets/1505860.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="03P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch-tact">
<description>&lt;b&gt;Diptronics THMD &amp; SMD tact switches&lt;/b&gt;
&lt;p&gt;&lt;ul&gt;
&lt;li&gt;DTS-3: 3.5x6mm THMD tact switch
&lt;li&gt;DTS-6, DTS-64: 6x6mm THMD tact switch
&lt;li&gt;DTSM-3: 3.5x6mm SMD tact switch
&lt;li&gt;DTSM-6, DTSM-64: 6x6mm SMD tact switch
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="DTS-6">
</package>
</packages>
</library>
<library name="diy-modules">
<description>&lt;b&gt;DIY Modules for Arduino, Raspberry Pi, CubieBoard etc.&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
The library contains a list of symbols and footprints for popular, cheap and easy-to-use electronic modules.&lt;br&gt;
The modules are intend to work with microprocessor-based platforms such as &lt;a href="http://arduino.cc"&gt;Arduino&lt;/a&gt;, &lt;a href="http://raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt;, &lt;a href="http://cubieboard.org/"&gt;CubieBoard&lt;/a&gt;, &lt;a href="http://beagleboard.org/"&gt;BeagleBone&lt;/a&gt; and many others. There are many manufacturers of the modules in the world. Almost all of them can be bought on &lt;a href="ebay.com"&gt;ebay.com&lt;/a&gt;.&lt;br&gt;
&lt;br&gt;
By using this library, you can design a PCB for devices created with usage of modules. Even if you do not need to create PCB design, you can also use the library to quickly document your work by drawing schematics of devices built by you.&lt;br&gt;
&lt;br&gt;
The latest version, examples, photos and much more can be found at: &lt;b&gt;&lt;a href="http://diymodules.org/eagle"&gt;diymodules.org/eagle&lt;/a&gt;&lt;/b&gt;&lt;br&gt;&lt;br&gt;
Comments, suggestions and bug reports please send to: &lt;b&gt;&lt;a href="mailto:eagle@diymodules.org"&gt;eagle@diymodules.org&lt;/b&gt;&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Version: 1.8.0 (2017-Jul-02)&lt;/i&gt;&lt;br&gt;
&lt;i&gt;Created by: Miroslaw Brudnowski&lt;/i&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Released under the Creative Commons Attribution 4.0 International License: &lt;a href="http://creativecommons.org/licenses/by/4.0"&gt;http://creativecommons.org/licenses/by/4.0&lt;/a&gt;&lt;/i&gt;
&lt;br&gt;&lt;br&gt;
&lt;center&gt;
&lt;a href="http://diymodules.org/eagle"&gt;&lt;img src="http://www.diymodules.org/img/diymodules-lbr-image.php?v=1.8.0" alt="DIYmodules.org"&gt;&lt;/a&gt;
&lt;/center&gt;</description>
<packages>
<package name="DISPLAY-OLED-128X32">
<description>&lt;b&gt;128x32 Dot Matrix OLED Module&lt;/b&gt; with &lt;b&gt;I2C&lt;/b&gt; interface</description>
</package>
</packages>
</library>
<library name="_hhn_attiny25_45_85">
<description>&lt;h3&gt;ATMEL ATtiny 25 / 45 /48&lt;/h3&gt;
&lt;p&gt;&lt;br /&gt;&lt;b&gt;&lt;u&gt;Supplied Packages:&lt;/u&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;P&lt;/b&gt; &amp;nbsp; = PDIP 08 30mil&lt;br /&gt;
&lt;b&gt;S&lt;/b&gt; &amp;nbsp; = SOIC 08 EIAJ 208mil&lt;br /&gt;
&lt;b&gt;SS&lt;/b&gt; = SOIC 08 JEDEC 150mil&lt;br /&gt;
&lt;b&gt;X&lt;/b&gt;&gt; &amp;nbsp; = TSSOP 08 4.4mm&lt;/p&gt;

&lt;p&gt;&lt;u&gt;&lt;b&gt;Revisions / Changelog&lt;/b&gt;&lt;/u&gt;&lt;br /&gt;
&amp;bull; &amp;nbsp;5.0.0 [EAGLE 5]&lt;br /&gt;
&lt;/p&gt;

&lt;hr /&gt;

&lt;author&gt;
&lt;p&gt;&lt;u&gt;Author:&lt;/u&gt;&lt;br /&gt;
Dipl.-Ing. FH Rainer Bayer&lt;br /&gt;
HHN Hochschule Heilbronn (Heilbronn University), &lt;i&gt;rainer.bayer@hs-heilbronn.de&lt;/i&gt;&lt;br /&gt;
Ingenieurbüro ing-rb, &lt;i&gt;mail@ing-rb.de&lt;/i&gt;&lt;/p&gt;&lt;/author&gt;</description>
<packages>
<package name="PDIP08_300MIL">
<description>&lt;b&gt;DIL08 300mil&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="G1" library="battery" package="CH291-1220LF" value="CH291-1220LF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="VALUE"/>
</element>
<element name="RELE" library="con-amp-quick" package="03P" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch-tact" package="DTS-6" value="DTS-6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="switch-tact" package="DTS-6" value="DTS-6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="diy-modules" package="DISPLAY-OLED-128X32" value="DISPLAY-OLED-128X32">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="_hhn_attiny25_45_85" package="PDIP08_300MIL" value="ATTINY85-20P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="S2" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="S1" pad="2"/>
<contactref element="G1" pad="-"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="3"/>
<contactref element="S2" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="2"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="G1" pad="+"/>
<contactref element="RELE" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="3"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="4"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="RELE" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
