<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="48.26" x2="0" y2="0" width="0" layer="20"/>
<text>P9-AiR</text>
<text>TJL-8/2015</text>
<text>NOT</text>
<text>P9-AiR</text>
<text>TJL-8/2015</text>
<text>BUFFER</text>
<wire x1="0" y1="0" x2="142.24" y2="0" width="0" layer="20"/>
<text>P9-AiR</text>
<text>TJL-8/2015</text>
<text>NAND</text>
<wire x1="142.24" y1="0" x2="142.24" y2="48.26" width="0" layer="20"/>
<wire x1="142.24" y1="48.26" x2="0" y2="48.26" width="0" layer="20"/>
<text>P9-AiR</text>
<text>TJL-8/2015</text>
<text>OR</text>
<text>P9-AiR</text>
<text>TJL-8/2015</text>
<text>AND</text>
<text>P9-AiR</text>
<text>TJL-8/2015</text>
<text>OR</text>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
</packages>
</library>
<library name="cellphone">
<packages>
<package name="BUTTON_6MM_JLEAD">
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="LED_1206">
<description>&lt;b&gt;CHICAGO MINIATURE LAMP, INC.&lt;/b&gt;&lt;p&gt;
7022X Series SMT LEDs 1206 Package Size</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-PTH-NS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="adafruit" package="M1206" value="10K"/>
<element name="S1" library="cellphone" package="BUTTON_6MM_JLEAD" value=""/>
<element name="LED1" library="eagle-ltspice" package="LED_1206" value="">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICETYPE" value="diode"/>
<attribute name="SPICEPREFIX" value="D"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="M1206" value="10K"/>
<element name="JP1" library="SparkFun-Connectors" package="JST-2-PTH-NS" value="M02-JST-2-PTH-NO_SILK"/>
<element name="N3" library="fab" package="SOT-23" value="N1">
<attribute name="NAME"/>
</element>
<element name="P3" library="fab" package="SOT-23" value="P1">
<attribute name="NAME"/>
</element>
<element name="R5" library="adafruit" package="M1206" value="10K"/>
<element name="S3" library="cellphone" package="BUTTON_6MM_JLEAD" value=""/>
<element name="LED3" library="eagle-ltspice" package="LED_1206" value="">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICETYPE" value="diode"/>
<attribute name="SPICEPREFIX" value="D"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="M1206" value="10K"/>
<element name="JP3" library="SparkFun-Connectors" package="JST-2-PTH-NS" value="M02-JST-2-PTH-NO_SILK"/>
<element name="N4" library="fab" package="SOT-23" value="N1">
<attribute name="NAME"/>
</element>
<element name="P4" library="fab" package="SOT-23" value="P1">
<attribute name="NAME"/>
</element>
<element name="N5" library="fab" package="SOT-23" value="N1">
<attribute name="NAME"/>
</element>
<element name="P5" library="fab" package="SOT-23" value="P1">
<attribute name="NAME"/>
</element>
<element name="N-1" library="fab" package="SOT-23" value="N1">
<attribute name="VALUE"/>
</element>
<element name="P-1" library="fab" package="SOT-23" value="P1">
<attribute name="VALUE"/>
</element>
<element name="N-2" library="fab" package="SOT-23" value="N2">
<attribute name="VALUE"/>
</element>
<element name="P-2" library="fab" package="SOT-23" value="P2">
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="M1206" value="10K"/>
<element name="R4" library="adafruit" package="M1206" value="10K"/>
<element name="S2" library="cellphone" package="BUTTON_6MM_JLEAD" value=""/>
<element name="S4" library="cellphone" package="BUTTON_6MM_JLEAD" value=""/>
<element name="LED2" library="eagle-ltspice" package="LED_1206" value="">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICETYPE" value="diode"/>
<attribute name="SPICEPREFIX" value="D"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="M1206" value="10K"/>
<element name="JP2" library="SparkFun-Connectors" package="JST-2-PTH-NS" value="M02-JST-2-PTH-NO_SILK"/>
<element name="N-3" library="fab" package="SOT-23" value="N1">
<attribute name="VALUE"/>
</element>
<element name="P-3" library="fab" package="SOT-23" value="P1">
<attribute name="VALUE"/>
</element>
<element name="N-4" library="fab" package="SOT-23" value="N2">
<attribute name="VALUE"/>
</element>
<element name="P-4" library="fab" package="SOT-23" value="P2">
<attribute name="VALUE"/>
</element>
<element name="R8" library="adafruit" package="M1206" value="10K"/>
<element name="R9" library="adafruit" package="M1206" value="10K"/>
<element name="S5" library="cellphone" package="BUTTON_6MM_JLEAD" value=""/>
<element name="S6" library="cellphone" package="BUTTON_6MM_JLEAD" value=""/>
<element name="LED4" library="eagle-ltspice" package="LED_1206" value="">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICETYPE" value="diode"/>
<attribute name="SPICEPREFIX" value="D"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="adafruit" package="M1206" value="10K"/>
<element name="JP4" library="SparkFun-Connectors" package="JST-2-PTH-NS" value="M02-JST-2-PTH-NO_SILK"/>
<element name="N1" library="fab" package="SOT-23" value="N1">
<attribute name="NAME"/>
</element>
<element name="P1" library="fab" package="SOT-23" value="P1">
<attribute name="NAME"/>
</element>
<element name="N-5" library="fab" package="SOT-23" value="N1">
<attribute name="VALUE"/>
</element>
<element name="P-5" library="fab" package="SOT-23" value="P1">
<attribute name="VALUE"/>
</element>
<element name="N-6" library="fab" package="SOT-23" value="N2">
<attribute name="VALUE"/>
</element>
<element name="P-6" library="fab" package="SOT-23" value="P2">
<attribute name="VALUE"/>
</element>
<element name="R11" library="adafruit" package="M1206" value="10K"/>
<element name="R12" library="adafruit" package="M1206" value="10K"/>
<element name="S7" library="cellphone" package="BUTTON_6MM_JLEAD" value=""/>
<element name="S8" library="cellphone" package="BUTTON_6MM_JLEAD" value=""/>
<element name="LED5" library="eagle-ltspice" package="LED_1206" value="">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICETYPE" value="diode"/>
<attribute name="SPICEPREFIX" value="D"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="adafruit" package="M1206" value="10K"/>
<element name="JP5" library="SparkFun-Connectors" package="JST-2-PTH-NS" value="M02-JST-2-PTH-NO_SILK"/>
<element name="N-7" library="fab" package="SOT-23" value="N1"/>
<element name="P-7" library="fab" package="SOT-23" value="P1"/>
<element name="N-8" library="fab" package="SOT-23" value="N1">
<attribute name="VALUE"/>
</element>
<element name="P-8" library="fab" package="SOT-23" value="P1">
<attribute name="VALUE"/>
</element>
<element name="N-9" library="fab" package="SOT-23" value="N2">
<attribute name="VALUE"/>
</element>
<element name="P-9" library="fab" package="SOT-23" value="P2">
<attribute name="VALUE"/>
</element>
<element name="R14" library="adafruit" package="M1206" value="10K"/>
<element name="R15" library="adafruit" package="M1206" value="10K"/>
<element name="S9" library="cellphone" package="BUTTON_6MM_JLEAD" value=""/>
<element name="S10" library="cellphone" package="BUTTON_6MM_JLEAD" value=""/>
<element name="LED6" library="eagle-ltspice" package="LED_1206" value="">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICETYPE" value="diode"/>
<attribute name="SPICEPREFIX" value="D"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="adafruit" package="M1206" value="10K"/>
<element name="JP6" library="SparkFun-Connectors" package="JST-2-PTH-NS" value="M02-JST-2-PTH-NO_SILK"/>
</elements>
<signals>
<signal name="OUT">
<contactref element="R2" pad="2"/>
<contactref element="P3" pad="1"/>
<contactref element="N3" pad="1"/>
</signal>
<signal name="VDD">
<contactref element="S1" pad="P$1"/>
<contactref element="S1" pad="P$2"/>
<contactref element="JP1" pad="2"/>
<contactref element="P3" pad="2"/>
</signal>
<signal name="VSS">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="JP1" pad="1"/>
<contactref element="N3" pad="2"/>
</signal>
<signal name="A">
<contactref element="R1" pad="1"/>
<contactref element="S1" pad="P$3"/>
<contactref element="S1" pad="P$4"/>
<contactref element="P3" pad="3"/>
<contactref element="N3" pad="3"/>
</signal>
<signal name="LED-IN">
<contactref element="LED1" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="OUT1">
<contactref element="R6" pad="2"/>
<contactref element="P4" pad="1"/>
<contactref element="N4" pad="1"/>
</signal>
<signal name="VDD1">
<contactref element="S3" pad="P$1"/>
<contactref element="S3" pad="P$2"/>
<contactref element="JP3" pad="2"/>
<contactref element="P4" pad="2"/>
<contactref element="P5" pad="2"/>
</signal>
<signal name="VSS1">
<contactref element="R5" pad="2"/>
<contactref element="LED3" pad="C"/>
<contactref element="JP3" pad="1"/>
<contactref element="N4" pad="2"/>
<contactref element="N5" pad="2"/>
</signal>
<signal name="A1">
<contactref element="R5" pad="1"/>
<contactref element="S3" pad="P$3"/>
<contactref element="S3" pad="P$4"/>
<contactref element="P5" pad="3"/>
<contactref element="N5" pad="3"/>
</signal>
<signal name="LED-IN2">
<contactref element="LED3" pad="A"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="INV-OUT1">
<contactref element="P5" pad="1"/>
<contactref element="N5" pad="1"/>
<contactref element="P4" pad="3"/>
<contactref element="N4" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="N-2" pad="1"/>
<contactref element="N-1" pad="2"/>
</signal>
<signal name="OUT2">
<contactref element="P-2" pad="1"/>
<contactref element="N-1" pad="1"/>
<contactref element="P-1" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="VDD2">
<contactref element="S2" pad="P$1"/>
<contactref element="S4" pad="P$1"/>
<contactref element="S2" pad="P$2"/>
<contactref element="S4" pad="P$2"/>
<contactref element="P-1" pad="2"/>
<contactref element="P-2" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="VSS2">
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="N-2" pad="2"/>
<contactref element="LED2" pad="C"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="A2">
<contactref element="R3" pad="1"/>
<contactref element="S2" pad="P$3"/>
<contactref element="S2" pad="P$4"/>
<contactref element="N-1" pad="3"/>
<contactref element="P-1" pad="3"/>
</signal>
<signal name="B">
<contactref element="R4" pad="1"/>
<contactref element="S4" pad="P$3"/>
<contactref element="S4" pad="P$4"/>
<contactref element="N-2" pad="3"/>
<contactref element="P-2" pad="3"/>
</signal>
<signal name="LED-IN1">
<contactref element="LED2" pad="A"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="OUT3">
<contactref element="R10" pad="2"/>
<contactref element="P1" pad="1"/>
<contactref element="N1" pad="1"/>
</signal>
<signal name="VDD3">
<contactref element="S5" pad="P$1"/>
<contactref element="S6" pad="P$1"/>
<contactref element="S5" pad="P$2"/>
<contactref element="S6" pad="P$2"/>
<contactref element="JP4" pad="2"/>
<contactref element="P1" pad="2"/>
<contactref element="P-3" pad="2"/>
</signal>
<signal name="VSS3">
<contactref element="R9" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="LED4" pad="C"/>
<contactref element="JP4" pad="1"/>
<contactref element="N1" pad="2"/>
<contactref element="N-3" pad="2"/>
<contactref element="N-4" pad="2"/>
</signal>
<signal name="A3">
<contactref element="R8" pad="1"/>
<contactref element="S5" pad="P$3"/>
<contactref element="S5" pad="P$4"/>
<contactref element="N-3" pad="3"/>
<contactref element="P-3" pad="3"/>
</signal>
<signal name="B1">
<contactref element="R9" pad="1"/>
<contactref element="S6" pad="P$3"/>
<contactref element="S6" pad="P$4"/>
<contactref element="N-4" pad="3"/>
<contactref element="P-4" pad="3"/>
</signal>
<signal name="LED-IN3">
<contactref element="LED4" pad="A"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="INV-IN">
<contactref element="P1" pad="3"/>
<contactref element="N1" pad="3"/>
<contactref element="N-3" pad="1"/>
<contactref element="N-4" pad="1"/>
<contactref element="P-4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="P-4" pad="2"/>
<contactref element="P-3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="N-6" pad="1"/>
<contactref element="N-5" pad="2"/>
</signal>
<signal name="OUT4">
<contactref element="R13" pad="2"/>
<contactref element="P-7" pad="1"/>
<contactref element="N-7" pad="1"/>
</signal>
<signal name="VDD4">
<contactref element="S7" pad="P$1"/>
<contactref element="S8" pad="P$1"/>
<contactref element="S7" pad="P$2"/>
<contactref element="S8" pad="P$2"/>
<contactref element="P-5" pad="2"/>
<contactref element="P-6" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="P-7" pad="2"/>
</signal>
<signal name="VSS4">
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="LED5" pad="C"/>
<contactref element="JP5" pad="1"/>
<contactref element="N-7" pad="2"/>
<contactref element="N-6" pad="2"/>
</signal>
<signal name="A4">
<contactref element="R11" pad="1"/>
<contactref element="S7" pad="P$3"/>
<contactref element="S7" pad="P$4"/>
<contactref element="N-5" pad="3"/>
<contactref element="P-5" pad="3"/>
</signal>
<signal name="B2">
<contactref element="R12" pad="1"/>
<contactref element="S8" pad="P$3"/>
<contactref element="S8" pad="P$4"/>
<contactref element="N-6" pad="3"/>
<contactref element="P-6" pad="3"/>
</signal>
<signal name="LED-IN4">
<contactref element="LED5" pad="A"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="INV-IN1">
<contactref element="P-6" pad="1"/>
<contactref element="N-5" pad="1"/>
<contactref element="P-5" pad="1"/>
<contactref element="P-7" pad="3"/>
<contactref element="N-7" pad="3"/>
</signal>
<signal name="OUT5">
<contactref element="R16" pad="2"/>
<contactref element="N-8" pad="1"/>
<contactref element="N-9" pad="1"/>
<contactref element="P-9" pad="1"/>
</signal>
<signal name="VDD5">
<contactref element="S9" pad="P$1"/>
<contactref element="S10" pad="P$1"/>
<contactref element="S9" pad="P$2"/>
<contactref element="S10" pad="P$2"/>
<contactref element="JP6" pad="2"/>
<contactref element="P-8" pad="2"/>
</signal>
<signal name="VSS5">
<contactref element="R15" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="LED6" pad="C"/>
<contactref element="JP6" pad="1"/>
<contactref element="N-8" pad="2"/>
<contactref element="N-9" pad="2"/>
</signal>
<signal name="A5">
<contactref element="R14" pad="1"/>
<contactref element="S9" pad="P$3"/>
<contactref element="S9" pad="P$4"/>
<contactref element="N-8" pad="3"/>
<contactref element="P-8" pad="3"/>
</signal>
<signal name="B3">
<contactref element="R15" pad="1"/>
<contactref element="S10" pad="P$3"/>
<contactref element="S10" pad="P$4"/>
<contactref element="N-9" pad="3"/>
<contactref element="P-9" pad="3"/>
</signal>
<signal name="LED-IN5">
<contactref element="LED6" pad="A"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="P-9" pad="2"/>
<contactref element="P-8" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
