<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.2">
<drawing>
<board>
<plain>
<wire x1="-0.254" y1="147.828" x2="-0.127" y2="22.319" width="0" layer="20"/>
<wire x1="-0.127" y1="22.319" x2="9.873" y2="12.319" width="0" layer="20" curve="90"/>
<wire x1="9.873" y1="12.319" x2="42.177" y2="12.446" width="0" layer="20"/>
<wire x1="42.177" y1="12.446" x2="52.177" y2="22.446" width="0" layer="20" curve="90"/>
<wire x1="52.177" y1="22.446" x2="52.05" y2="147.828" width="0" layer="20"/>
<wire x1="52.05" y1="147.828" x2="42.05" y2="160.198" width="0" layer="20" curve="90"/>
<wire x1="42.05" y1="160.198" x2="9.746" y2="160.198" width="0" layer="20"/>
<wire x1="9.746" y1="160.198" x2="-0.254" y2="147.828" width="0" layer="20" curve="90"/>
<hole x="4.953" y="19.812" drill="5.08"/>
<hole x="44.196" y="153.67" drill="5.08"/>
<hole x="6.477" y="153.289" drill="5.08"/>
<hole x="47.498" y="20.193" drill="5.08"/>
</plain>
<libraries>
<library name="Paul_Custom">
<packages>
<package name="CFP3_SOD123W_NEX">
</package>
<package name="DIO_PDZVTFT_ROM">
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="IND_7447709680_WRE">
</package>
<package name="MOSFET_BSC039N06NSATMA1">
</package>
<package name="MICROBUILDER_JSTPH2">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
<package name="C2220K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2220 reflow solder&lt;/b&gt;&lt;p&gt;Metric Code Size 5650</description>
</package>
<package name="MICROBUILDER_CHIPLED_0805_NOOUTLINE">
</package>
<package name="VREG_UWS-5/10-Q48N-C">
</package>
<package name="SOT230P700X180-3N">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="SPARKFUN_QFN-16_0.5MM">
<description>&lt;h3&gt;QFN-16 0.5mm Pitch&lt;/h3&gt;
3 x 3mm Outline&lt;br&gt;
16-pin&lt;br&gt;
Used on the MMA8452Q accelerometer&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Unproven&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Layout in accordance with App note AN4077&lt;br&gt;
http://cache.freescale.com/files/sensors/doc/app_note/AN4077.pdf</description>
</package>
<package name="CUI_PJ-202AH">
</package>
<package name="TSR2-SINGLE_TRP">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="microbuilder">
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="WROOM32_SKINNY">
</package>
<package name="RESPACK_4X0603">
</package>
<package name="0603-NO">
</package>
<package name="CHIPLED_0805_NOOUTLINE">
</package>
<package name="0805-NO">
</package>
<package name="QFN24_4MM_SMSC">
</package>
<package name="4UCONN_20329_V2">
</package>
<package name="SOD-123">
<description>&lt;b&gt;SOD-123&lt;/b&gt;
&lt;p&gt;Source: http://www.diodes.com/datasheets/ds30139.pdf&lt;/p&gt;</description>
</package>
<package name="SOT23-R">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Reflow soldering</description>
</package>
<package name="BTN_KMR2_4.6X2.8">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-SMD">
<description>&lt;h3&gt;JST-Right Angle Male Header SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;li&gt;JST_2MM_MALE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CR1" library="Paul_Custom" package="CFP3_SOD123W_NEX" value="PMEG4030ER,115">
<attribute name="BUILT_BY" value="EMA_Cory"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="https://assets.nexperia.com/documents/data-sheet/PMEG4030ER.pdf"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="PMEG4030ER,115"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="Nexperia_2020-05-11"/>
<attribute name="VENDOR" value="Nexperia"/>
</element>
<element name="CR2" library="Paul_Custom" package="CFP3_SOD123W_NEX" value="PMEG4030ER,115">
<attribute name="BUILT_BY" value="EMA_Cory"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="https://assets.nexperia.com/documents/data-sheet/PMEG4030ER.pdf"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="PMEG4030ER,115"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="Nexperia_2020-05-11"/>
<attribute name="VENDOR" value="Nexperia"/>
</element>
<element name="R1" library="Paul_Custom" package="DIO_PDZVTFT_ROM" value="PDZVTR16A">
<attribute name="BUILT_BY" value="EMA_Matt"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="PDZVTR16A"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="Rohm_2019-09-23"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="ROHM Semiconductor"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Paul_Custom" package="DIO_PDZVTFT_ROM" value="PDZVTR16A">
<attribute name="BUILT_BY" value="EMA_Matt"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="PDZVTR16A"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="Rohm_2019-09-23"/>
<attribute name="VENDOR" value="ROHM Semiconductor"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="Paul_Custom" package="C0805" value="">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Paul_Custom" package="C0805" value="">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="Paul_Custom" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="Paul_Custom" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="Paul_Custom" package="IND_7447709680_WRE" value="7447709680">
<attribute name="BUILT_BY" value="EMA_Cory"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="https://www.we-online.de/katalog/datasheet/7447709680.pdf"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="7447709680"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="Wurth_Electronics_2020-04-27"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="Wurth Electronics"/>
</element>
<element name="L3" library="Paul_Custom" package="IND_7447709680_WRE" value="7447709680">
<attribute name="BUILT_BY" value="EMA_Cory"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="https://www.we-online.de/katalog/datasheet/7447709680.pdf"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="7447709680"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="Wurth_Electronics_2020-04-27"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="Wurth Electronics"/>
</element>
<element name="Q3" library="Paul_Custom" package="MOSFET_BSC039N06NSATMA1" value="BSC039N06NSATMA1">
<attribute name="DESCRIPTION" value=" OptiMOS 5 60V is optimized for synchronous rectification in switched mode power supplies (SMPS) such as those found in servers and desktops and tablet charger. In addition these devices are a perfect choice for a broad range of industrial applications including motor control, solar micro inverter and fast switching DC-DC converter. "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="BSC039N06NSATMA1CT-ND"/>
<attribute name="MF" value="Infineon Technologies"/>
<attribute name="MP" value="BSC039N06NSATMA1"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="PowerTDFN-8 Infineon"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/BSC039N06NSATMA1/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="Paul_Custom" package="MOSFET_BSC039N06NSATMA1" value="BSC039N06NSATMA1">
<attribute name="DESCRIPTION" value=" OptiMOS 5 60V is optimized for synchronous rectification in switched mode power supplies (SMPS) such as those found in servers and desktops and tablet charger. In addition these devices are a perfect choice for a broad range of industrial applications including motor control, solar micro inverter and fast switching DC-DC converter. "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="BSC039N06NSATMA1CT-ND"/>
<attribute name="MF" value="Infineon Technologies"/>
<attribute name="MP" value="BSC039N06NSATMA1"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="PowerTDFN-8 Infineon"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/BSC039N06NSATMA1/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="Paul_Custom" package="MICROBUILDER_JSTPH2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="Paul_Custom" package="C2220K" value="">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="Paul_Custom" package="C2220K" value="">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="Paul_Custom" package="MICROBUILDER_CHIPLED_0805_NOOUTLINE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D9" library="Paul_Custom" package="MICROBUILDER_CHIPLED_0805_NOOUTLINE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun" package="SOT23-3" value="mmbt2222">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="SparkFun" package="SOT23-3" value="mmbt2222">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="microbuilder" package="WROOM32_SKINNY" value="ESP32_WROOM32_SKINNY">
<attribute name="SPICEPREFIX" value="X"/>
</element>
<element name="R2" library="microbuilder" package="RESPACK_4X0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="microbuilder" package="CHIPLED_0805_NOOUTLINE" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="microbuilder" package="0603-NO" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="microbuilder" package="QFN24_4MM_SMSC" value="CP2104">
<attribute name="NAME"/>
</element>
<element name="X4" library="microbuilder" package="4UCONN_20329_V2" value="20329">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="microbuilder" package="0805-NO" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="microbuilder" package="0805-NO" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="microbuilder" package="0603-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="microbuilder" package="0805-NO" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="microbuilder" package="SOD-123" value="MBR120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="microbuilder" package="0805-NO" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="microbuilder" package="SOT23-R" value="DMG3415U">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="microbuilder" package="0603-NO" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW2" library="microbuilder" package="BTN_KMR2_4.6X2.8" value="KMR2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="microbuilder" package="0603-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Paul_Custom" package="VREG_UWS-5/10-Q48N-C" value="UWS-5/10-Q48N-C">
<attribute name="DESCRIPTION" value=" Isolated Module DC DC Converter 1 Output 5V 10A 18V - 75V Input "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="811-2361-ND"/>
<attribute name="MF" value="Murata Power"/>
<attribute name="MP" value="UWS-5/10-Q48N-C"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="DIP-8 Murata Power"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/UWS-5/10-Q48N-C/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="Paul_Custom" package="SOT230P700X180-3N" value="SPX1117M3-L-3-3/TR">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value=" Linear Voltage Regulator IC 1 Output 800mA SOT-223 "/>
<attribute name="MF" value="MaxLinear, Inc."/>
<attribute name="MP" value="SPX1117M3-L-3-3/TR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-223 Exar"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/SPX1117M3-L-3-3/TR/?ref=eda"/>
</element>
<element name="C3" library="microbuilder" package="0603-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="Paul_Custom" package="C1206" value="">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="microbuilder" package="0603-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="Paul_Custom" package="C1206" value="">
<attribute name="NAME"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X03" value="455-1750-1-ND">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="XXX-00000"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X03" value="455-1750-1-ND">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="XXX-00000"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="microbuilder" package="0603-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="microbuilder" package="0805-NO" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="microbuilder" package="0603-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="microbuilder" package="0805-NO" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="33"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="33"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="Paul_Custom" package="SPARKFUN_QFN-16_0.5MM" value="SPARKFUN_MMA8452Q">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="microbuilder" package="0603-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="microbuilder" package="0805-NO" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="microbuilder" package="0603-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="Paul_Custom" package="CUI_PJ-202AH" value="PJ-202AH">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="CUI_PURCHASE_URL" value="https://www.cuidevices.com/product/interconnect/connectors/dc-power-connectors/jacks/pj-202ah?utm_source=snapeda.com&amp;utm_medium=referral&amp;utm_campaign=snapedaBOM"/>
<attribute name="DESCRIPTION" value="2.0 x 6.5 mm, 5.0 A, Horizontal, Through Hole, Kinked Pins, Dc Power Jack Connector"/>
<attribute name="MF" value="CUI Devices"/>
<attribute name="MP" value="PJ-202AH"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/PJ-202AH/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="microbuilder" package="0603-NO" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="JST-2-SMD" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="JST-2-SMD" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="VALUE"/>
</element>
<element name="RLA1" library="Paul_Custom" package="TSR2-SINGLE_TRP" value="TSR_2-2450">
<attribute name="BUILT_BY" value="EMA_Justin"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="https://www.tracopower.com/products/tsr2.pdf"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="TSR 2-2450"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="Traco_Power_2020-06-03"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="Traco Power"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="X2" pad="1"/>
<contactref element="X2" pad="P$1"/>
<contactref element="X2" pad="15"/>
<contactref element="X2" pad="38"/>
<contactref element="D3" pad="C"/>
<contactref element="IC1" pad="2"/>
<contactref element="X4" pad="BASE@2"/>
<contactref element="X4" pad="SPRT@1"/>
<contactref element="X4" pad="SPRT@2"/>
<contactref element="X4" pad="SPRT@3"/>
<contactref element="X4" pad="BASE@1"/>
<contactref element="X4" pad="GND"/>
<contactref element="X4" pad="SPRT@4"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="THERM"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="SW2" pad="A"/>
<contactref element="SW2" pad="A'"/>
<contactref element="C9" pad="2"/>
<contactref element="D8" pad="C"/>
<contactref element="D9" pad="C"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="C12" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="3"/>
<contactref element="C16" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="U4" pad="12"/>
<contactref element="U4" pad="10"/>
<contactref element="U4" pad="5"/>
<contactref element="C20" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="3"/>
<contactref element="C22" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="RLA1" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="X2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="5"/>
<contactref element="C7" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="U4" pad="14"/>
<contactref element="C19" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="C22" pad="1"/>
<contactref element="R2" pad="6"/>
</signal>
<signal name="N$10">
<contactref element="R9" pad="1"/>
<contactref element="D8" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="R10" pad="1"/>
<contactref element="D9" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="Q3" pad="4"/>
<contactref element="R1" pad="1"/>
<contactref element="CR1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="CR1" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="L3" pad="1"/>
<contactref element="Q4" pad="7"/>
<contactref element="Q4" pad="5"/>
<contactref element="Q4" pad="8"/>
<contactref element="Q4" pad="6"/>
<contactref element="Q4" pad="9"/>
<contactref element="C14" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="SJ2" pad="1"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R3" pad="1"/>
<contactref element="CR2" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="Q4" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="C2" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="CR2" pad="1"/>
<contactref element="Q3" pad="7"/>
<contactref element="Q3" pad="5"/>
<contactref element="Q3" pad="8"/>
<contactref element="Q3" pad="6"/>
<contactref element="Q3" pad="9"/>
<contactref element="L2" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="SJ1" pad="1"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="WPT_VDD">
<contactref element="L2" pad="1"/>
<contactref element="L3" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="C10" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="Q2" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="RLA1" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="Q1" pad="3"/>
<contactref element="X2" pad="3"/>
<contactref element="SW2" pad="B'"/>
<contactref element="SW2" pad="B"/>
<contactref element="C9" pad="1"/>
<contactref element="R2" pad="3"/>
</signal>
<signal name="GPIO0">
<contactref element="Q5" pad="3"/>
<contactref element="X2" pad="25"/>
</signal>
<signal name="RXD0">
<contactref element="X2" pad="34"/>
<contactref element="IC1" pad="21"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="TXD0">
<contactref element="X2" pad="35"/>
<contactref element="IC1" pad="20"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="RTS">
<contactref element="Q1" pad="2"/>
<contactref element="R2" pad="7"/>
<contactref element="IC1" pad="19"/>
</signal>
<signal name="DTR">
<contactref element="Q5" pad="2"/>
<contactref element="R2" pad="4"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="N$12">
<contactref element="Q1" pad="1"/>
<contactref element="R2" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="Q5" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="X2" pad="30"/>
</signal>
<signal name="A5_IO4">
<contactref element="X2" pad="26"/>
</signal>
<signal name="SDA">
<contactref element="X2" pad="37"/>
<contactref element="U4" pad="6"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="X2" pad="36"/>
<contactref element="U4" pad="4"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="IO33_A9">
<contactref element="X2" pad="9"/>
</signal>
<signal name="IO32_A7">
<contactref element="X2" pad="8"/>
</signal>
<signal name="IO27_A10">
<contactref element="X2" pad="12"/>
</signal>
<signal name="MISO">
<contactref element="X2" pad="31"/>
</signal>
<signal name="SCK">
<contactref element="X2" pad="29"/>
</signal>
<signal name="A4_IO36">
<contactref element="X2" pad="4"/>
</signal>
<signal name="A3_I39">
<contactref element="X2" pad="5"/>
</signal>
<signal name="A2_I34">
<contactref element="X2" pad="6"/>
</signal>
<signal name="A13_I35">
<contactref element="X2" pad="7"/>
</signal>
<signal name="IO12_A11">
<contactref element="X2" pad="14"/>
</signal>
<signal name="IO21">
<contactref element="X2" pad="33"/>
</signal>
<signal name="IO14_A6">
<contactref element="X2" pad="13"/>
</signal>
<signal name="VBUS">
<contactref element="IC1" pad="8"/>
<contactref element="X4" pad="VBUS"/>
<contactref element="R16" pad="2"/>
<contactref element="D4" pad="A"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R8" pad="2"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="X4" pad="D+"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="X4" pad="D-"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="N$18">
<contactref element="C6" pad="1"/>
<contactref element="D4" pad="C"/>
<contactref element="Q2" pad="2"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="WPT_ENABLE">
<contactref element="U1" pad="2"/>
<contactref element="X2" pad="23"/>
</signal>
<signal name="AGND">
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q4" pad="1"/>
<contactref element="Q4" pad="3"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q3" pad="1"/>
<contactref element="Q3" pad="3"/>
<contactref element="U1" pad="4"/>
<contactref element="C10" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="LINK_ESTABLISHED">
<contactref element="X2" pad="16"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="SERV0">
<contactref element="J1" pad="1"/>
<contactref element="X2" pad="27"/>
</signal>
<signal name="SERV1">
<contactref element="J2" pad="1"/>
<contactref element="X2" pad="28"/>
</signal>
<signal name="WPT_TRIM">
<contactref element="U1" pad="6"/>
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="WPT_-SENSE">
<contactref element="R12" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="WPT_+SENSE">
<contactref element="R11" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="SERV_ENABLE">
<contactref element="X2" pad="10"/>
</signal>
<signal name="COILV_A">
<contactref element="SJ1" pad="2"/>
<contactref element="X2" pad="11"/>
</signal>
<signal name="COILV_B">
<contactref element="X2" pad="24"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="C21" pad="1"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U4" pad="7"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="J1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="RLA1" pad="3"/>
<contactref element="J4" pad="1"/>
<contactref element="J5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
