<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="-1.5" y1="15.5" x2="3.5" y2="10.5" width="0" layer="20"/>
<wire x1="3.5" y1="10.5" x2="62.5" y2="10.5" width="0" layer="20"/>
<wire x1="62.5" y1="10.5" x2="67.5" y2="15.5" width="0" layer="20"/>
<wire x1="67.5" y1="15.5" x2="67.5" y2="74.5" width="0" layer="20"/>
<wire x1="67.5" y1="74.5" x2="62.5" y2="79.5" width="0" layer="20"/>
<wire x1="62.5" y1="79.5" x2="3.5" y2="79.5" width="0" layer="20"/>
<wire x1="3.5" y1="79.5" x2="-1.5" y2="74.5" width="0" layer="20"/>
<wire x1="-1.5" y1="74.5" x2="-1.5" y2="15.5" width="0" layer="20"/>
</plain>
<libraries>
<library name="thar">
<packages>
<package name="WS2812B_WIRE2">
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$3" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$4" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$5" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$6" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$7" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$8" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$9" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$10" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$11" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$12" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$13" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$14" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$15" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$16" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$17" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="U$18" library="thar" package="WS2812B_WIRE2" value="WS2812BWIRE2"/>
<element name="JP1" library="pinhead" package="1X02" value=""/>
<element name="JP6" library="pinhead" package="1X02" value=""/>
<element name="JP7" library="pinhead" package="1X02" value=""/>
<element name="JP8" library="pinhead" package="1X02" value=""/>
<element name="C1" library="thar" package="1206" value="100n"/>
<element name="C2" library="thar" package="1206" value="100n"/>
<element name="C3" library="thar" package="1206" value="100n"/>
<element name="C4" library="thar" package="1206" value="100n"/>
<element name="C5" library="thar" package="1206" value="100n"/>
<element name="C6" library="thar" package="1206" value="100n"/>
<element name="C7" library="thar" package="1206" value="100n"/>
<element name="C8" library="thar" package="1206" value="100n"/>
<element name="C9" library="thar" package="1206" value="100n"/>
<element name="C10" library="thar" package="1206" value="100n"/>
<element name="C11" library="thar" package="1206" value="100n"/>
<element name="C12" library="thar" package="1206" value="100n"/>
<element name="C13" library="thar" package="1206" value="100n"/>
<element name="C14" library="thar" package="1206" value="100n"/>
<element name="C15" library="thar" package="1206" value="100n"/>
<element name="C16" library="thar" package="1206" value="100n"/>
<element name="R1" library="thar" package="1206" value=""/>
<element name="C18" library="thar" package="1206" value="100n"/>
<element name="C20" library="thar" package="1206" value="10µ"/>
<element name="U1" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="Tiny45-20-SMT">
<attribute name="PROD_ID" value="IC-08922"/>
</element>
<element name="JP2" library="pinhead" package="1X06" value=""/>
<element name="JP3" library="pinhead" package="1X02" value=""/>
<element name="JP4" library="pinhead" package="1X02" value=""/>
<element name="JP5" library="pinhead" package="1X02" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$3" pad="P$5"/>
<contactref element="U$4" pad="P$5"/>
<contactref element="U$5" pad="P$5"/>
<contactref element="U$6" pad="P$5"/>
<contactref element="U$10" pad="P$5"/>
<contactref element="U$9" pad="P$5"/>
<contactref element="U$8" pad="P$5"/>
<contactref element="U$7" pad="P$5"/>
<contactref element="U$11" pad="P$5"/>
<contactref element="U$12" pad="P$5"/>
<contactref element="U$13" pad="P$5"/>
<contactref element="U$14" pad="P$5"/>
<contactref element="U$18" pad="P$5"/>
<contactref element="U$17" pad="P$5"/>
<contactref element="U$16" pad="P$5"/>
<contactref element="U$15" pad="P$5"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP7" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="R1" pad="1"/>
<contactref element="JP2" pad="5"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$15" pad="P$7"/>
<contactref element="U$16" pad="P$7"/>
<contactref element="U$17" pad="P$7"/>
<contactref element="U$18" pad="P$7"/>
<contactref element="U$14" pad="P$7"/>
<contactref element="U$13" pad="P$7"/>
<contactref element="U$12" pad="P$7"/>
<contactref element="U$11" pad="P$7"/>
<contactref element="U$7" pad="P$7"/>
<contactref element="U$8" pad="P$7"/>
<contactref element="U$9" pad="P$7"/>
<contactref element="U$10" pad="P$7"/>
<contactref element="U$6" pad="P$7"/>
<contactref element="U$5" pad="P$7"/>
<contactref element="U$4" pad="P$7"/>
<contactref element="U$3" pad="P$7"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="JP8" pad="2"/>
<contactref element="JP6" pad="2"/>
<contactref element="C18" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="JP2" pad="6"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$3" pad="P$6"/>
<contactref element="U$4" pad="P$8"/>
</signal>
<signal name="N$2">
<contactref element="U$4" pad="P$6"/>
<contactref element="U$5" pad="P$8"/>
</signal>
<signal name="N$3">
<contactref element="U$5" pad="P$6"/>
<contactref element="U$6" pad="P$8"/>
</signal>
<signal name="N$4">
<contactref element="U$9" pad="P$6"/>
<contactref element="U$10" pad="P$8"/>
</signal>
<signal name="N$5">
<contactref element="U$8" pad="P$6"/>
<contactref element="U$9" pad="P$8"/>
</signal>
<signal name="N$6">
<contactref element="U$7" pad="P$6"/>
<contactref element="U$8" pad="P$8"/>
</signal>
<signal name="N$7">
<contactref element="U$11" pad="P$6"/>
<contactref element="U$12" pad="P$8"/>
</signal>
<signal name="N$8">
<contactref element="U$12" pad="P$6"/>
<contactref element="U$13" pad="P$8"/>
</signal>
<signal name="N$9">
<contactref element="U$13" pad="P$6"/>
<contactref element="U$14" pad="P$8"/>
</signal>
<signal name="N$10">
<contactref element="U$17" pad="P$6"/>
<contactref element="U$18" pad="P$8"/>
</signal>
<signal name="N$11">
<contactref element="U$16" pad="P$6"/>
<contactref element="U$17" pad="P$8"/>
</signal>
<signal name="N$12">
<contactref element="U$15" pad="P$6"/>
<contactref element="U$16" pad="P$8"/>
</signal>
<signal name="N$13">
<contactref element="U$6" pad="P$6"/>
<contactref element="U$7" pad="P$8"/>
</signal>
<signal name="N$14">
<contactref element="U$10" pad="P$6"/>
<contactref element="U$11" pad="P$8"/>
</signal>
<signal name="N$15">
<contactref element="U$14" pad="P$6"/>
<contactref element="U$15" pad="P$8"/>
</signal>
<signal name="RST">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="5"/>
<contactref element="U$3" pad="P$8"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="6"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="7"/>
<contactref element="JP8" pad="1"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="2"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="N$19">
</signal>
<signal name="N$20">
</signal>
<signal name="N$21">
</signal>
<signal name="N$16">
</signal>
</signals>
</board>
</drawing>
</eagle>
