**F450 KK 2.1.5 DOCUMENTATION FUTURE 2.0**

**Physical Connections:**

*Reciever to Flight Controller:*

* Channel 1-5 Signal to Signal of KK 2.1.5
* Channel 1 +ve to KK +ve & Channel 1 -ve to KK -ve

(Positive in the center row, negative in the last row and signal in the first row of the receiver)

*Motors to Flight Controller:*

* 1st Leg: Top Left
* 2nd Leg: Top Right Signal KK 2.1
* 3rd Leg: Down Right
* 4th Leg: Down Left

*ESC Connections:*

* Negative Row to Corresponding Wire
* Positive Row to Corresponding Wire
* Center Wire Signal

*Propellor Spinning:*

CW & CW Top Left and Down Right

CCW & CCW Top Right and Down left