<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="22.86" y1="30.48" x2="25.4" y2="30.48" width="0.1524" layer="20"/>
<wire x1="54.61" y1="27.94" x2="54.61" y2="11.43" width="0.1524" layer="20"/>
<wire x1="54.61" y1="11.43" x2="55.88" y2="10.16" width="0.1524" layer="20"/>
<wire x1="55.88" y1="10.16" x2="55.88" y2="5.08" width="0.1524" layer="20"/>
<wire x1="55.88" y1="5.08" x2="53.34" y2="2.54" width="0.1524" layer="20"/>
<wire x1="53.34" y1="2.54" x2="45.72" y2="2.54" width="0.1524" layer="20"/>
<wire x1="15.24" y1="7.62" x2="15.24" y2="22.86" width="0.1524" layer="20"/>
<wire x1="15.24" y1="22.86" x2="22.86" y2="30.48" width="0.1524" layer="20" curve="-90"/>
<wire x1="15.24" y1="7.62" x2="20.32" y2="2.54" width="0.1524" layer="20" curve="90"/>
<wire x1="25.4" y1="30.48" x2="27.94" y2="27.94" width="0.1524" layer="20" curve="90"/>
<wire x1="27.94" y1="27.94" x2="54.61" y2="27.94" width="0.1524" layer="20"/>
<wire x1="20.32" y1="2.54" x2="33.02" y2="2.54" width="0.1524" layer="20"/>
<wire x1="33.02" y1="2.54" x2="35.56" y2="0" width="0.1524" layer="20"/>
<wire x1="35.56" y1="0" x2="43.18" y2="0" width="0.1524" layer="20"/>
<wire x1="43.18" y1="0" x2="45.72" y2="2.54" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="CR2032-THRU">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 220 Vertical&lt;/b&gt; Package works with various parts including N-Channel MOSFET SparkFun SKU: COM-10213</description>
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="DIP254P762X533-8">
</package>
</packages>
</library>
<library name="switch">
<description>&lt;b&gt;Switches&lt;/b&gt;&lt;p&gt;
Marquardt, Siemens, C&amp;K, ITT, and others&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="255SB">
<description>&lt;b&gt;SLIDING SWITCH&lt;/b&gt;&lt;p&gt;
distributor Buerklin, 11G810</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C025-024X044" value=""/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO220V" value="24A/20V/50mΩ">
<attribute name="PROD_ID" value="TRANS-13060"/>
</element>
<element name="R4" library="adafruit" package="0204V" value=""/>
<element name="U$1" library="adafruit" package="CR2032-THRU" value=""/>
<element name="U1" library="Atmel_By_element14_Batch_1-00" package="DIP254P762X533-8" value="ATTINY85-20PU">
<attribute name="MPN" value="ATTINY85-20PU"/>
<attribute name="OC_FARNELL" value="1455162"/>
<attribute name="OC_NEWARK" value="58M3796"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="Atmel"/>
</element>
<element name="S1" library="switch" package="255SB" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="Q1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="Q1" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="-"/>
<contactref element="Q1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="S1" pad="2"/>
<contactref element="U$1" pad="+1"/>
</signal>
<signal name="N$2">
</signal>
</signals>
</board>
</drawing>
</eagle>
