[{"id":"29ff67ae.ff61c8","type":"ibmiot in","z":"effab020.87b3","authentication":"boundService","apiKey":"","inputType":"evt","deviceId":"ESP8266","applicationId":"","deviceType":"ESP8266","eventType":"+","commandType":"","format":"json","name":"IBM IoT","service":"registered","allDevices":false,"allApplications":"","allDeviceTypes":false,"allEvents":true,"allCommands":"","allFormats":"","qos":0,"x":218,"y":233,"wires":[["3b62857c.e6f80a"]]},{"id":"1f50d080.1fc08","type":"debug","z":"effab020.87b3","name":"","active":true,"console":"false","complete":"false","x":565,"y":362,"wires":[]},{"id":"3b62857c.e6f80a","type":"function","z":"effab020.87b3","name":"","func":"return {payload:msg.payload.d.weight};","outputs":1,"noerr":0,"x":359,"y":151,"wires":[["1f50d080.1fc08","34ec3240.f855ce"]]},{"id":"34ec3240.f855ce","type":"ui_gauge","z":"effab020.87b3","name":"","group":"881ed2d1.5dcd7","order":0,"width":0,"height":0,"gtype":"gage","title":"IoT Scale","label":"grams","format":"{{value | number:1}}g","min":0,"max":"5000","colors":["#00b500","#e6e600","#ca3838"],"x":600,"y":246,"wires":[]},{"id":"881ed2d1.5dcd7","type":"ui_group","z":"","name":"Weight","tab":"acd7764d.c49d68","disp":true,"width":"6"},{"id":"acd7764d.c49d68","type":"ui_tab","z":"","name":"Weight","icon":"dashboard"}]