(export (version D)
  (design
    (source C:/Users/Catalin/Documents/HUB/Hub.sch)
    (date "30.04.2017 23:16:30")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Hub.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J5)
      (value USB_A)
      (footprint Connectors:USB_A)
      (libsource (lib conn) (part USB_A))
      (sheetpath (names /) (tstamps /))
      (tstamp 5905F932))
    (comp (ref J6)
      (value USB_A)
      (footprint Connectors:USB_A)
      (libsource (lib conn) (part USB_A))
      (sheetpath (names /) (tstamps /))
      (tstamp 5905FB99))
    (comp (ref J3)
      (value USB_A)
      (footprint Connectors:USB_A)
      (libsource (lib conn) (part USB_A))
      (sheetpath (names /) (tstamps /))
      (tstamp 5905FCF0))
    (comp (ref J2)
      (value USB_A)
      (footprint Connectors:USB_A)
      (libsource (lib conn) (part USB_A))
      (sheetpath (names /) (tstamps /))
      (tstamp 5905FD5D))
    (comp (ref J4)
      (value USB_A)
      (footprint Connectors:USB_A)
      (libsource (lib conn) (part USB_A))
      (sheetpath (names /) (tstamps /))
      (tstamp 5905FDC0))
    (comp (ref R5)
      (value 100)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59063F2F))
    (comp (ref R1)
      (value 100)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59063FB6))
    (comp (ref R2)
      (value 100)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5906401F))
    (comp (ref R3)
      (value 100)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 590640AE))
    (comp (ref R4)
      (value 100)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59064154))
    (comp (ref J1)
      (value Screw_Terminal_1x02)
      (footprint Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol)
      (libsource (lib conn) (part Screw_Terminal_1x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 59064B2E)))
  (libparts
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part Screw_Terminal_1x02)
      (description "2-pin screw terminal connector")
      (footprints
        (fp bornier2)
        (fp TerminalBlock*2pol))
      (fields
        (field (name Reference) J)
        (field (name Value) Screw_Terminal_1x02))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part USB_A)
      (description "USB Type A connector")
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_A))
      (pins
        (pin (num 1) (name VBUS) (type power_in))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name Shield) (type passive)))))
  (libraries
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib")))
  (nets
    (net (code 1) (name "Net-(J6-Pad3)")
      (node (ref J6) (pin 3))
      (node (ref R1) (pin 1)))
    (net (code 2) (name "Net-(J2-Pad3)")
      (node (ref J2) (pin 3))
      (node (ref R3) (pin 1)))
    (net (code 3) (name "Net-(J3-Pad2)")
      (node (ref R2) (pin 2))
      (node (ref J3) (pin 2)))
    (net (code 4) (name "Net-(J3-Pad3)")
      (node (ref R2) (pin 1))
      (node (ref J3) (pin 3)))
    (net (code 5) (name "Net-(J6-Pad2)")
      (node (ref R1) (pin 2))
      (node (ref J6) (pin 2)))
    (net (code 6) (name "Net-(J5-Pad2)")
      (node (ref J5) (pin 2))
      (node (ref R5) (pin 2)))
    (net (code 7) (name "Net-(J5-Pad3)")
      (node (ref J5) (pin 3))
      (node (ref R5) (pin 1)))
    (net (code 8) (name "Net-(J4-Pad2)")
      (node (ref J4) (pin 2))
      (node (ref R4) (pin 2)))
    (net (code 9) (name "Net-(J4-Pad3)")
      (node (ref J4) (pin 3))
      (node (ref R4) (pin 1)))
    (net (code 10) (name "Net-(J2-Pad2)")
      (node (ref J2) (pin 2))
      (node (ref R3) (pin 2)))
    (net (code 11) (name GND)
      (node (ref J2) (pin 4))
      (node (ref J3) (pin 4))
      (node (ref J6) (pin 4))
      (node (ref J5) (pin 4))
      (node (ref J4) (pin 4))
      (node (ref J1) (pin 2)))
    (net (code 12) (name VCC)
      (node (ref J5) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref J4) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref J3) (pin 1))
      (node (ref J6) (pin 1)))
    (net (code 13) (name "Net-(J3-Pad5)")
      (node (ref J3) (pin 5)))
    (net (code 14) (name "Net-(J4-Pad5)")
      (node (ref J4) (pin 5)))
    (net (code 15) (name "Net-(J2-Pad5)")
      (node (ref J2) (pin 5)))
    (net (code 16) (name "Net-(J6-Pad5)")
      (node (ref J6) (pin 5)))
    (net (code 17) (name "Net-(J5-Pad5)")
      (node (ref J5) (pin 5)))))