<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="25.4" width="0.2032" layer="20"/>
<wire x1="0" y1="25.4" x2="25.4" y2="25.4" width="0.2032" layer="20"/>
<wire x1="25.4" y1="25.4" x2="25.4" y2="0" width="0.2032" layer="20"/>
<wire x1="25.4" y1="0" x2="0" y2="0" width="0.2032" layer="20"/>
<text>3.3V</text>
<text>SDA</text>
<text>SCL</text>
<text>GND</text>
<text>ADDR
Open-0x69
Close-0x68</text>
<text>3.3V</text>
<text>SDA</text>
<text>SCL</text>
<text>GND</text>
<text>GridEYE</text>
<text>v10</text>
<text>GridEYE
8x8 IR Array</text>
<text>INT</text>
<text>INT</text>
<text>N. Seidle</text>
<text>A. England</text>
<text>Units in Inches</text>
<text>I2C
PU</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="MICRO-FIDUCIAL">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_3_2-NC_PASTE_SILK">
</package>
</packages>
</library>
<library name="SparkX">
<packages>
<package name="1X04_1MM_RA">
<description>&lt;h3&gt;SMD- 4 Pin Right Angle &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
<description>&lt;h3&gt;Creative Commons License Template&lt;/h3&gt;
&lt;p&gt;CC BY-SA 4.0 License with &lt;a href="https://creativecommons.org/licenses/by-sa/4.0/"&gt;link to license&lt;/a&gt; and placeholder for designer name.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FRAME_LEDGER&lt;/li&gt;
&lt;li&gt;FRAME_LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="OSHW-LOGO-MINI">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Mini - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SFE_LOGO_NAME_.1">
<description>&lt;h3&gt;SparkFun Font Logo - 0.1" Height - Silkscreen&lt;/h3&gt;
&lt;p&gt;SparkFun font logo&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;SFE_LOGO_NAME&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SFE_LOGO_NAME_FLAME_.1">
<description>&lt;h3&gt;SparkFun Font Logo w/ Flame - 0.1" Height - Silkscreen&lt;/h3&gt;
&lt;p&gt;SparkFun font logo with flame logo&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;SFE_LOGO_NAME_FLAME&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="REVISION">
<description>&lt;h3&gt;"Revision By" Text - tDoc&lt;/h3&gt;
&lt;p&gt;Preceding text for revisor documentation.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;REVISION&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Sensors&lt;/h3&gt;
This library contains sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="GRIDEYE-AMG88">
<description>&lt;h3&gt;Panasonic AMG8833 GRIDEye&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 10&lt;/li&gt;
&lt;li&gt;Pin pitch: .050 in.&lt;/li&gt;
&lt;li&gt;Area: .315 in. x 11.6 in.&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=https://cdn.sparkfun.com/assets/2/c/9/d/8/Grid-EYE_Datasheet.pdf&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP3" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP4" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="SJ1" library="SparkFun" package="SJ_2S-NO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="JP6" library="SparkFun" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="R4" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07857"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07857"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun-Jumpers" package="SMT-JUMPER_3_2-NC_PASTE_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkX" package="1X04_1MM_RA" value="SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkX" package="1X04_NO_SILK" value="PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="U$2" library="SparkFun-Aesthetics" package="SFE_LOGO_NAME_FLAME_.1" value="SFE_LOGO_NAME_FLAME.1_INCH"/>
<element name="C4" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkX" package="1X04_1MM_RA" value="SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-MINI" value="OSHW-LOGOMINI"/>
<element name="U$1" library="SparkFun-Aesthetics" package="SFE_LOGO_NAME_.1" value="SFE_LOGO_NAME.1_INCH"/>
<element name="U2" library="SparkFun-Sensors" package="GRIDEYE-AMG88" value="GRIDEYE">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-13912"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603" value="2.2uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-07888"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="20">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07862"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="JP5" library="SparkFun" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="LOGO2" library="SparkFun-Aesthetics" package="REVISION" value="REVISION"/>
</elements>
<signals>
<signal name="3.3V">
<contactref element="JP7" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="J4" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="9"/>
<contactref element="U2" pad="13"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="SJ1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="J4" pad="1"/>
<contactref element="U2" pad="6"/>
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="R4" pad="1"/>
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="4"/>
<contactref element="J4" pad="4"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="R5" pad="1"/>
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="3"/>
<contactref element="J4" pad="3"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="ADDR">
<contactref element="SJ1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="R5" pad="2"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R4" pad="2"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="INT">
<contactref element="U2" pad="4"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="12"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="10"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
