<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<packages>
<package name="SMA">
<description>&lt;b&gt;SMA&lt;/b&gt; CASE 403D-02&lt;p&gt;
Source: http://www.onsemi.com/pub_link/Collateral/MBRA340T3-D.PDF</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="D">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PNP">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="1N4001" prefix="D">
<description>1N4001 Diode: Vreverse = 50V, Vforward = 1V, Iavg = 1A, SMA Footprint (https://www.onsemi.com/pub/Collateral/1N4001-D.PDF)</description>
<gates>
<gate name="G$1" symbol="D"/>
</gates>
<devices>
<device name="" package="SMA">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N3906" prefix="Q">
<description>2N3906 pnp transistor, SOT-23 Package. Typical marking: 2A (https://www.onsemi.com/pub/Collateral/MMBT3906LT1-D.PDF)</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
