<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="34.75" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="52.5" y2="0" width="0" layer="20"/>
<wire x1="52.5" y1="34.75" x2="0" y2="34.75" width="0" layer="20"/>
<text>VCC</text>
<text>RESET</text>
<text>A0</text>
<text>CS</text>
<text>SDA</text>
<text>SCK</text>
<text>LED</text>
<text>160x128 TFT display</text>
<text>GND</text>
<text>(ST7735)</text>
<hole x="2.55" y="31.625" drill="3.2"/>
<hole x="2.55" y="3.125" drill="3.2"/>
<wire x1="52.5" y1="0" x2="52.5" y2="13" width="0" layer="20"/>
<wire x1="52.5" y1="13" x2="39.5" y2="13" width="0" layer="20"/>
<wire x1="39.5" y1="13" x2="39.5" y2="21.5" width="0" layer="20"/>
<wire x1="39.5" y1="21.5" x2="52.5" y2="21.5" width="0" layer="20"/>
<wire x1="52.5" y1="34.75" x2="52.5" y2="21.5" width="0" layer="20"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="JD-T1800">
</package>
<package name="1X08-BIG">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="adafruit" package="JD-T1800" value="JD-T1800"/>
<element name="R1" library="SparkFun-Passives" package="1206" value="22 ohm">
<attribute name="NAME"/>
</element>
<element name="C1" library="rcl" package="C0805K" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="JP1" library="adafruit" package="1X08-BIG" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="7"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="9"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="8"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="+3V3">
<contactref element="U1" pad="10"/>
<contactref element="U1" pad="11"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="DC">
<contactref element="U1" pad="7"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="CS">
<contactref element="U1" pad="12"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="6"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="LED">
<contactref element="JP1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
