<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="48.768" y2="0" width="0" layer="20"/>
<wire x1="48.768" y1="0" x2="48.768" y2="26.924" width="0" layer="20"/>
<wire x1="48.768" y1="26.924" x2="0" y2="26.924" width="0" layer="20"/>
<wire x1="0" y1="26.924" x2="0" y2="0" width="0" layer="20"/>
<text>LED1</text>
<text>LED2</text>
<text>LED4</text>
<text>C1</text>
<text>C2</text>
<text>C3</text>
<text>R3</text>
<text>R1</text>
<text>R4</text>
<text>R6</text>
<text>R5</text>
<text>R2</text>
<text>1</text>
<text>10</text>
<text>20</text>
<text>11</text>
<text>FTD232R</text>
<text>GND</text>
<text>CTS</text>
<text>VCC</text>
<text>TXO</text>
<text>RXI</text>
<text>RTS</text>
<text>XBuddy</text>
<text>Ver 0.3</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="E2,5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="SFE_41310">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="XBEE-1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="adafruit" package="C025-025X050" value="0.1uF"/>
<element name="C1" library="adafruit" package="C025-025X050" value="0.1uF"/>
<element name="U1" library="SparkFun" package="SSOP28DB" value="FT232RLSSOP"/>
<element name="R1" library="adafruit" package="0204/5" value="1K"/>
<element name="R2" library="adafruit" package="0204/5" value="1K"/>
<element name="JP1" library="SparkFun" package="1X06" value=""/>
<element name="X1" library="SFE_41310" package="USB-A-H" value="USB-A-H"/>
<element name="U$5" library="SFE_41310" package="XBEE-1" value="XBEE-1B1"/>
<element name="R3" library="adafruit" package="0204/5" value="1K"/>
<element name="LED4" library="adafruit" package="LED3MM" value="Red"/>
<element name="R4" library="adafruit" package="0204/5" value="1K"/>
<element name="R5" library="adafruit" package="0204/5" value="10"/>
<element name="R6" library="adafruit" package="0204/5" value="10"/>
<element name="LED1" library="adafruit" package="LED3MM" value="Red"/>
<element name="LED2" library="adafruit" package="LED3MM" value="Green"/>
<element name="LED3" library="adafruit" package="LED3MM" value="Green"/>
<element name="C3" library="adafruit" package="E2,5-6" value="10uF"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="25"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="21"/>
<contactref element="JP1" pad="6"/>
<contactref element="R3" pad="1"/>
<contactref element="U$5" pad="10"/>
<contactref element="R4" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="-"/>
<contactref element="X1" pad="GND"/>
</signal>
<signal name="USB_D-">
<contactref element="U1" pad="16"/>
<contactref element="X1" pad="D-"/>
</signal>
<signal name="USB_D+">
<contactref element="U1" pad="15"/>
<contactref element="X1" pad="D+"/>
</signal>
<signal name="CTS">
<contactref element="JP1" pad="5"/>
<contactref element="U$5" pad="16"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="DTR">
<contactref element="U1" pad="2"/>
</signal>
<signal name="TXO">
<contactref element="JP1" pad="3"/>
<contactref element="U$5" pad="3"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="RXI">
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="U$5" pad="2"/>
</signal>
<signal name="5V">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="4"/>
<contactref element="U1" pad="20"/>
<contactref element="X1" pad="VBUS"/>
<contactref element="C3" pad="+"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$5" pad="15"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="LED4" pad="K"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="RTS">
<contactref element="U$5" pad="12"/>
<contactref element="U1" pad="3"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R6" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="TXLED">
<contactref element="U1" pad="23"/>
<contactref element="LED1" pad="K"/>
</signal>
<signal name="RXLED">
<contactref element="U1" pad="22"/>
<contactref element="LED2" pad="K"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$5" pad="7"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="LED3" pad="K"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="17"/>
<contactref element="U$5" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
