<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="65.71" y2="0" width="0" layer="20"/>
<wire x1="65.71" y1="0" x2="65.71" y2="38.725" width="0" layer="20"/>
<wire x1="65.71" y1="38.725" x2="0" y2="38.725" width="0" layer="20"/>
<wire x1="0" y1="38.725" x2="0" y2="0" width="0" layer="20"/>
<text>DMX_IN</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>5V</text>
<text>GND</text>
<text>12V</text>
<text>DMX LED Strip Controller    V1</text>
<text>Design by Matthew Tong    9 June 2014</text>
<text>GND</text>
<hole x="3.4925" y="31.75" drill="2.2"/>
<hole x="2.8575" y="2.8575" drill="2.2"/>
<hole x="60.6425" y="3.175" drill="2.2"/>
<hole x="62.865" y="34.925" drill="2.2"/>
<text>SCK</text>
<text>MISO</text>
<text>MOSI</text>
<text>RST</text>
<text>.1</text>
</plain>
<libraries>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SOT23-W">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Wave soldering</description>
</package>
<package name="CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_LOCK">
</package>
<package name="1X05">
</package>
<package name="MOLEX-1X3">
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="QFP80P900X900X120-32N">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="LED-TRICOLOR-SMD">
</package>
</packages>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-4">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="dc-dc-converter">
<description>&lt;b&gt;DC-DC Converters&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="NME">
<description>&lt;b&gt;DC-DC CONVERTER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC2" library="74xx-eu" package="DIL16" value="74HC595N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="3166028"/>
<attribute name="MF" value="NXP"/>
<attribute name="MPN" value="74HC595N"/>
</element>
<element name="IC1" library="74xx-eu" package="DIL16" value="74HC595N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="3166028"/>
<attribute name="MF" value="NXP"/>
<attribute name="MPN" value="74HC595N"/>
</element>
<element name="Q15" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q14" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q13" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="RGB_5" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q12" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q11" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q10" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="RGB_4" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q9" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q8" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q7" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="RGB_3" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q6" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q5" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q4" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="RGB_2" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q3" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q2" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="Q1" library="adafruit" package="SOT23-W" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="RGB_1" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="U2" library="Atmel_By_element14_Batch_1" package="QFP80P900X900X120-32N" value="ATMEGA328P-AU">
<attribute name="PACKAGE" value="TQFP-32"/>
<attribute name="OC_NEWARK" value="14R4631"/>
<attribute name="MPN" value="ATMEGA328P-AU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1715486"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MF" value="ATMEL"/>
</element>
<element name="Q16" library="adafruit" package="CTS406" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C102" library="SparkFun" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="1740665"/>
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="08053C104KAT2A"/>
</element>
<element name="C103" library="SparkFun" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="1740665"/>
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="08053C104KAT2A"/>
</element>
<element name="C1" library="SparkFun" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="1740665"/>
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="08053C104KAT2A"/>
</element>
<element name="C100" library="SparkFun" package="0805" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="2280675"/>
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="08055A220JAT2A"/>
</element>
<element name="C101" library="SparkFun" package="0805" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="2280675"/>
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="08055A220JAT2A"/>
</element>
<element name="R1" library="SparkFun" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="1577673"/>
<attribute name="MF" value="PANASONIC"/>
<attribute name="MPN" value="ERA6AEB103V"/>
</element>
<element name="ICSP" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="U1" library="SparkFun" package="SOT23-5" value="MIC5205">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="1556768"/>
<attribute name="MF" value="MICREL SEMICONDUCTOR"/>
<attribute name="MPN" value="MIC5205-5.0YM5 TR"/>
</element>
<element name="C4" library="SparkFun" package="0805" value="470pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="499195"/>
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="08051A471JAT2A"/>
</element>
<element name="C5" library="SparkFun" package="0805" value="2.2pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="1856195"/>
<attribute name="MF" value="MULTICOMP"/>
<attribute name="MPN" value="MCMT21N2R2C160CT"/>
</element>
<element name="POWER_IN" library="con-wago-500" package="W237-4" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="SparkFun-DigitalIC" package="DIL08" value="MAX485DIL">
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="OK1" library="optocoupler" package="DIL08" value="6N137">
<attribute name="OC_NEWARK" value="52M1895"/>
<attribute name="MPN" value="6N137"/>
<attribute name="MF" value="VISHAY"/>
<attribute name="OC_FARNELL" value="1328376"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DMX_IN" library="SparkFun-Connectors" package="MOLEX-1X3" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R3" library="SparkFun" package="0805" value="470">
<attribute name="OC_FARNELL" value="1811902"/>
<attribute name="MF" value="KOA"/>
<attribute name="MPN" value="RK73H2ATTD4700F"/>
</element>
<element name="R2" library="SparkFun" package="0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="1469923"/>
<attribute name="MF" value="VISHAY DRALORIC"/>
<attribute name="MPN" value="CRCW08054K70FKEA"/>
</element>
<element name="STATUS" library="SparkFun" package="LED-TRICOLOR-SMD" value="LED-TRICOLOR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R6" library="SparkFun" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="1811839"/>
<attribute name="MF" value="KOA"/>
<attribute name="MPN" value="RK73H2ATTD2200F"/>
</element>
<element name="NME1" library="dc-dc-converter" package="NME" value="">
<attribute name="OC_NEWARK" value="98B8198"/>
<attribute name="MPN" value="NME0505SC"/>
<attribute name="MF" value="MURATA POWER SOLUTIONS"/>
<attribute name="OC_FARNELL" value="1021456"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="1740665"/>
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="08053C104KAT2A"/>
</element>
<element name="C3" library="SparkFun" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="1740665"/>
<attribute name="MF" value="AVX"/>
<attribute name="MPN" value="08053C104KAT2A"/>
</element>
<element name="R5" library="SparkFun" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="1811839"/>
<attribute name="MF" value="KOA"/>
<attribute name="MPN" value="RK73H2ATTD2200F"/>
</element>
<element name="R4" library="SparkFun" package="0805" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="1811839"/>
<attribute name="MF" value="KOA"/>
<attribute name="MPN" value="RK73H2ATTD2200F"/>
</element>
<element name="C6" library="SparkFun" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_FARNELL" value="1288204"/>
<attribute name="MF" value="KEMET"/>
<attribute name="MPN" value="C0805C106K4PACTU"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC2" pad="8"/>
<contactref element="IC1" pad="8"/>
<contactref element="Q15" pad="2"/>
<contactref element="Q14" pad="2"/>
<contactref element="Q13" pad="2"/>
<contactref element="IC2" pad="13"/>
<contactref element="C103" pad="1"/>
<contactref element="IC1" pad="13"/>
<contactref element="C1" pad="1"/>
<contactref element="Q12" pad="2"/>
<contactref element="Q11" pad="2"/>
<contactref element="Q10" pad="2"/>
<contactref element="Q9" pad="2"/>
<contactref element="Q8" pad="2"/>
<contactref element="Q7" pad="2"/>
<contactref element="Q6" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="C101" pad="2"/>
<contactref element="C100" pad="2"/>
<contactref element="U2" pad="21"/>
<contactref element="C102" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="ICSP" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="POWER_IN" pad="3"/>
<contactref element="POWER_IN" pad="2"/>
<contactref element="OK1" pad="5"/>
<contactref element="NME1" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="IC2" pad="16"/>
<contactref element="IC1" pad="16"/>
<contactref element="C103" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC2" pad="10"/>
<contactref element="C102" pad="2"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="C5" pad="1"/>
<contactref element="OK1" pad="8"/>
<contactref element="R2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="NME1" pad="2"/>
<contactref element="STATUS" pad="A"/>
</signal>
<signal name="AVCC">
<contactref element="U2" pad="18"/>
</signal>
<signal name="R1">
<contactref element="IC2" pad="15"/>
<contactref element="Q15" pad="1"/>
</signal>
<signal name="G1">
<contactref element="IC2" pad="1"/>
<contactref element="Q14" pad="1"/>
</signal>
<signal name="B1">
<contactref element="IC2" pad="2"/>
<contactref element="Q13" pad="1"/>
</signal>
<signal name="R2">
<contactref element="IC2" pad="3"/>
<contactref element="Q12" pad="1"/>
</signal>
<signal name="G2">
<contactref element="IC2" pad="4"/>
<contactref element="Q11" pad="1"/>
</signal>
<signal name="B2">
<contactref element="IC2" pad="5"/>
<contactref element="Q10" pad="1"/>
</signal>
<signal name="R3">
<contactref element="IC2" pad="6"/>
<contactref element="Q9" pad="1"/>
</signal>
<signal name="G3">
<contactref element="IC2" pad="7"/>
<contactref element="Q8" pad="1"/>
</signal>
<signal name="B3">
<contactref element="IC1" pad="15"/>
<contactref element="Q7" pad="1"/>
</signal>
<signal name="R4">
<contactref element="IC1" pad="1"/>
<contactref element="Q6" pad="1"/>
</signal>
<signal name="G4">
<contactref element="IC1" pad="2"/>
<contactref element="Q5" pad="1"/>
</signal>
<signal name="B4">
<contactref element="IC1" pad="3"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="R5">
<contactref element="IC1" pad="4"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="G5">
<contactref element="IC1" pad="5"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="B5">
<contactref element="IC1" pad="6"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="Q13" pad="3"/>
<contactref element="RGB_5" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="Q14" pad="3"/>
<contactref element="RGB_5" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="RGB_5" pad="2"/>
<contactref element="Q15" pad="3"/>
</signal>
<signal name="+12V">
<contactref element="RGB_5" pad="1"/>
<contactref element="RGB_4" pad="1"/>
<contactref element="RGB_3" pad="1"/>
<contactref element="RGB_2" pad="1"/>
<contactref element="RGB_1" pad="1"/>
<contactref element="POWER_IN" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="IC2" pad="9"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="LATCH">
<contactref element="IC1" pad="12"/>
<contactref element="IC2" pad="12"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="N$5">
<contactref element="Q10" pad="3"/>
<contactref element="RGB_4" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="Q11" pad="3"/>
<contactref element="RGB_4" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="RGB_4" pad="2"/>
<contactref element="Q12" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="Q7" pad="3"/>
<contactref element="RGB_3" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="Q8" pad="3"/>
<contactref element="RGB_3" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="RGB_3" pad="2"/>
<contactref element="Q9" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="Q4" pad="3"/>
<contactref element="RGB_2" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="Q5" pad="3"/>
<contactref element="RGB_2" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="RGB_2" pad="2"/>
<contactref element="Q6" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="Q1" pad="3"/>
<contactref element="RGB_1" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="Q2" pad="3"/>
<contactref element="RGB_1" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="RGB_1" pad="2"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="U2" pad="15"/>
<contactref element="ICSP" pad="2"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="RESET">
<contactref element="U2" pad="29"/>
<contactref element="R1" pad="1"/>
<contactref element="ICSP" pad="5"/>
</signal>
<signal name="MISO">
<contactref element="U2" pad="16"/>
<contactref element="ICSP" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="U2" pad="17"/>
<contactref element="ICSP" pad="4"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="XTAL2">
<contactref element="U2" pad="7"/>
<contactref element="C101" pad="1"/>
<contactref element="Q16" pad="1"/>
<contactref element="C100" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="Q16" pad="3"/>
</signal>
<signal name="RX">
<contactref element="U2" pad="30"/>
<contactref element="R2" pad="2"/>
<contactref element="OK1" pad="6"/>
</signal>
<signal name="TX">
<contactref element="U2" pad="31"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="4"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="POWER_IN" pad="1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="DMX_IN" pad="3"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="N$20">
<contactref element="IC3" pad="6"/>
<contactref element="DMX_IN" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="IC3" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="R3" pad="1"/>
<contactref element="OK1" pad="3"/>
</signal>
<signal name="N$27">
<contactref element="IC3" pad="8"/>
<contactref element="OK1" pad="2"/>
<contactref element="NME1" pad="4"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="U2" pad="9"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="U2" pad="10"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="R4" pad="2"/>
<contactref element="STATUS" pad="G"/>
</signal>
<signal name="N$30">
<contactref element="R5" pad="2"/>
<contactref element="STATUS" pad="B"/>
</signal>
<signal name="N$31">
<contactref element="R6" pad="2"/>
<contactref element="STATUS" pad="R"/>
</signal>
<signal name="STAT_G">
<contactref element="U2" pad="13"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="IC3" pad="2"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC3" pad="5"/>
<contactref element="DMX_IN" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="NME1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
