<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="65.71" y2="0" width="0" layer="20"/>
<wire x1="65.71" y1="0" x2="65.71" y2="35.55" width="0" layer="20"/>
<wire x1="65.71" y1="35.55" x2="0" y2="35.55" width="0" layer="20"/>
<wire x1="0" y1="35.55" x2="0" y2="0" width="0" layer="20"/>
<text>AQUATHUMB</text>
<text>v.1</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-2.5MM-6.5MM">
<description>2.5 mm spaced PTHs with 6.5 mm diameter outline</description>
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="78XXS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="317TS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL04">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
</packages>
</library>
<library name="triac">
<description>&lt;b&gt;Thyristors, Triacs, Trigger Diodes&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT82S">
<description>&lt;b&gt;SOT 82&lt;/b&gt; vertical (Cathode; Anode; Gate)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-6.5MM" value="100uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08439"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="v-reg" package="78XXS" value="LM7805">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="v-reg" package="317TS" value="LM317">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02" value="Header Alarm In">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02" value="Header Alarm Stop">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X02" value="Battery In">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X02" value="Header Micro Switch">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X03" value="Header Speed Potentiometer">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X02" value="Header Servo">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OK1" library="optocoupler" package="DIL04" value="PC817">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9707727"/>
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="VALUE"/>
</element>
<element name="OK2" library="optocoupler" package="DIL04" value="PC817">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PC817X4J000F"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9707727"/>
<attribute name="OC_NEWARK" value="97K7059"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0207/10" value="820">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0207/10" value="820">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0207/10" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="triac" package="SOT82S" value="2p4m">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T2" library="triac" package="SOT82S" value="2p4m">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="2"/>
<contactref element="T1" pad="G"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="T1" pad="C"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="OK1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="OK2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="OK2" pad="4"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="J2" pad="2"/>
<contactref element="OK2" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="OK1" pad="4"/>
<contactref element="T2" pad="G"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="T2" pad="C"/>
<contactref element="IC1" pad="IN"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="OUT"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="R3" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="IC2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="J6" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="OK1" pad="3"/>
<contactref element="J3" pad="1"/>
<contactref element="T1" pad="A"/>
<contactref element="T2" pad="A"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J4" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="J6" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="OK2" pad="2"/>
<contactref element="OK1" pad="2"/>
<contactref element="J5" pad="3"/>
<contactref element="IC1" pad="GND"/>
<contactref element="J4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
