<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="40.8549625" x2="0" y2="2.83980625" width="0.4064" layer="20"/>
<wire x1="0" y1="2.83980625" x2="2.83980625" y2="0" width="0.4064" layer="20" curve="90"/>
<wire x1="2.83980625" y1="0" x2="63.16108125" y2="0" width="0.4064" layer="20"/>
<wire x1="63.16108125" y1="0" x2="65.71" y2="2.54891875" width="0.4064" layer="20" curve="90"/>
<wire x1="65.71" y1="2.54891875" x2="65.71" y2="40.47101875" width="0.4064" layer="20"/>
<wire x1="65.71" y1="40.47101875" x2="61.74101875" y2="43.17" width="0.4064" layer="20" curve="90"/>
<wire x1="61.74101875" y1="43.17" x2="3.5850375" y2="43.17" width="0.4064" layer="20"/>
<wire x1="3.5850375" y1="43.17" x2="0" y2="40.8549625" width="0.4064" layer="20" curve="90"/>
<text>&lt;- USB</text>
<text>SPACE/ENTER</text>
<text>DOT</text>
<text>BACKSPACE</text>
<text>RETURN</text>
<text>DASH</text>
<text>&lt;- RIGHT HAND</text>
<text>LEFT HAND -&gt;</text>
<text>Inspired by Dot-dash coder (CO-3B, MX-4495)</text>
<text>^ Remove jumper for left hand operation</text>
</plain>
<libraries>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X12">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="RETURN" library="SparkFun-Retired" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="BACKSPACE" library="SparkFun-Retired" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="DASH" library="SparkFun-Retired" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="DOT" library="SparkFun-Retired" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="SPACE/ENTER" library="SparkFun-Retired" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="ALT" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CTRL" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FN" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SHIFT" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X12" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X12" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="RETURN" pad="2"/>
<contactref element="RETURN" pad="1"/>
<contactref element="BACKSPACE" pad="2"/>
<contactref element="BACKSPACE" pad="1"/>
<contactref element="DASH" pad="2"/>
<contactref element="DASH" pad="1"/>
<contactref element="DOT" pad="2"/>
<contactref element="DOT" pad="1"/>
<contactref element="SPACE/ENTER" pad="2"/>
<contactref element="SPACE/ENTER" pad="1"/>
<contactref element="SHIFT" pad="K"/>
<contactref element="FN" pad="K"/>
<contactref element="CTRL" pad="K"/>
<contactref element="ALT" pad="K"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="10"/>
<contactref element="J2" pad="9"/>
<contactref element="J3" pad="11"/>
</signal>
<signal name="PIN3_INT0">
<contactref element="J2" pad="7"/>
<contactref element="BACKSPACE" pad="4"/>
<contactref element="BACKSPACE" pad="3"/>
</signal>
<signal name="PIN2_INT1">
<contactref element="J2" pad="8"/>
<contactref element="DASH" pad="4"/>
<contactref element="DASH" pad="3"/>
</signal>
<signal name="PIN0_INT2">
<contactref element="J2" pad="11"/>
<contactref element="DOT" pad="4"/>
<contactref element="DOT" pad="3"/>
</signal>
<signal name="PIN1_INT3">
<contactref element="J2" pad="12"/>
<contactref element="SPACE/ENTER" pad="4"/>
<contactref element="SPACE/ENTER" pad="3"/>
</signal>
<signal name="PIN7_INT4">
<contactref element="J2" pad="3"/>
<contactref element="RETURN" pad="4"/>
<contactref element="RETURN" pad="3"/>
</signal>
<signal name="PIN10">
<contactref element="J3" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="PIN16">
<contactref element="J3" pad="2"/>
<contactref element="SHIFT" pad="A"/>
</signal>
<signal name="PIN14">
<contactref element="J3" pad="3"/>
<contactref element="FN" pad="A"/>
</signal>
<signal name="PIN15">
<contactref element="J3" pad="4"/>
<contactref element="CTRL" pad="A"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="PIN18">
<contactref element="J3" pad="5"/>
<contactref element="ALT" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
