<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="10.16" y1="36.83" x2="40.62" y2="36.83" width="0" layer="20"/>
<wire x1="40.62" y1="36.83" x2="40.62" y2="73.33" width="0" layer="20"/>
<wire x1="40.62" y1="73.33" x2="10.16" y2="73.33" width="0" layer="20"/>
<wire x1="10.16" y1="73.33" x2="10.16" y2="36.83" width="0" layer="20"/>
<text>RabbitCreek Design</text>
<text>ALASKA</text>
<text>ALASKA</text>
<text>RabbitCreek Design</text>
<text>RabbitCreek Design</text>
</plain>
<libraries>
<library name="SparkFun-Batteries">
<description>&lt;h3&gt;SparkFun Batteries&lt;/h3&gt;
This library contains battery clips, connectors, and appropriately sized silk outlines for LiPo batteries. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCOM_20MM_PTH">
<description>&lt;h3&gt;20mm (CR2032) Coin Cell Battery Holder - PTH&lt;/h3&gt;
&lt;p&gt;Basic 20mm coin cell holder. Posts can be inserted into 0.1" perf board! Holds the common CR2032 type batteries.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Prototyping/CoinCellHolder-20mm.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electromechanical Parts&lt;/h3&gt;
This library contains electromechanical devices, like motors, speakers,servos, and relays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BUZZER-12MM">
<description>&lt;h3&gt;12mm Buzzer - PTH&lt;/h3&gt;
&lt;p&gt;This is a small 12mm round speaker that operates around the audible 2kHz range. You can use these speakers to create simple music or user interfaces.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/General/cem-1203-42-.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BUZZER&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="switch">
<description>&lt;b&gt;Switches&lt;/b&gt;&lt;p&gt;
Marquardt, Siemens, C&amp;K, ITT, and others&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="320-916">
<description>&lt;b&gt;TOGGLE SWITCH&lt;/b&gt;&lt;p&gt;
distributor RS Components</description>
</package>
</packages>
</library>
<library name="mp3v50004">
<packages>
<package name="MP3V5004">
</package>
</packages>
</library>
<library name="_hhn_attiny25_45_85">
<description>&lt;h3&gt;ATMEL ATtiny 25 / 45 /48&lt;/h3&gt;
&lt;p&gt;&lt;br /&gt;&lt;b&gt;&lt;u&gt;Supplied Packages:&lt;/u&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;P&lt;/b&gt; &amp;nbsp; = PDIP 08 30mil&lt;br /&gt;
&lt;b&gt;S&lt;/b&gt; &amp;nbsp; = SOIC 08 EIAJ 208mil&lt;br /&gt;
&lt;b&gt;SS&lt;/b&gt; = SOIC 08 JEDEC 150mil&lt;br /&gt;
&lt;b&gt;X&lt;/b&gt;&gt; &amp;nbsp; = TSSOP 08 4.4mm&lt;/p&gt;

&lt;p&gt;&lt;u&gt;&lt;b&gt;Revisions / Changelog&lt;/b&gt;&lt;/u&gt;&lt;br /&gt;
&amp;bull; &amp;nbsp;5.0.0 [EAGLE 5]&lt;br /&gt;
&lt;/p&gt;

&lt;hr /&gt;

&lt;author&gt;
&lt;p&gt;&lt;u&gt;Author:&lt;/u&gt;&lt;br /&gt;
Dipl.-Ing. FH Rainer Bayer&lt;br /&gt;
HHN Hochschule Heilbronn (Heilbronn University), &lt;i&gt;rainer.bayer@hs-heilbronn.de&lt;/i&gt;&lt;br /&gt;
Ingenieurbüro ing-rb, &lt;i&gt;mail@ing-rb.de&lt;/i&gt;&lt;/p&gt;&lt;/author&gt;</description>
<packages>
<package name="PDIP08_300MIL">
<description>&lt;b&gt;DIL08 300mil&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BT1" library="SparkFun-Batteries" package="BATTCOM_20MM_PTH" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="BATT-09031"/>
<attribute name="SF_SKU" value="PRT-00783"/>
<attribute name="VALUE"/>
</element>
<element name="LS1" library="SparkFun-Electromechanical" package="BUZZER-12MM" value="BUZZER-PTH">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="COMP-08253"/>
<attribute name="SF_SKU" value="COM-07950"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch" package="320-916" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="mp3v50004" package="MP3V5004" value="">
<attribute name="NAME"/>
</element>
<element name="U1" library="_hhn_attiny25_45_85" package="PDIP08_300MIL" value="ATTINY85-20P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="S1" pad="3"/>
<contactref element="U1" pad="8"/>
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="S1" pad="2"/>
<contactref element="BT1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="LS1" pad="-"/>
<contactref element="BT1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P$4"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="5"/>
<contactref element="LS1" pad="+"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
